DICOM PS3.16 2019a - Content Mapping Resource

TID 5203 Echo Measurement (Current)
Prev | Echocardiography Procedure Report Templates | Next

### TID 5203 Echo Measurement

Table TID 5203. Parameters

Parameter Name | Parameter Usage
--- | ---
$Measurement | Coded term or Context Group for Concept Name of measurement
$Method | Value for Measurement Method

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 5203. Echo Measurement

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = $Measurement $Method = $Method $TargetSite = BCID 12236 “Echo Anatomic Sites” $TargetSiteMod = BCID 12237 “Echocardiography Anatomic Site Modifiers”
2 | > | HAS CONCEPT MOD | CODE | EV (G-C048, SRT, "Flow Direction") | 1 | U |  | BCID 12221 “Flow Direction”
3 | > | HAS CONCEPT MOD | CODE | EV (R-40899, SRT, "Respiratory Cycle Point") | 1 | U |  | DCID 12234 “Respiration State”
4 | > | HAS CONCEPT MOD | CODE | EV (R-4089A, SRT, "Cardiac Cycle Point") | 1 | U |  | DCID 12233 “Cardiac Phase”
5 | > | HAS ACQ CONTEXT | CODE | EV (G-0373, SRT, "Image Mode") | 1 | U |  | DCID 12224 “Ultrasound Image Modes”
6 | > | HAS ACQ CONTEXT | CODE | EV (111031, DCM, "Image View") | 1 | U |  | BCID 12226 “Echocardiography Image View”
7 | > | HAS ACQ CONTEXT | CODE | EV (18139-6, LN, "Stage") | 1 | U |  | BCID 12002 “Ultrasound Protocol Stage Types”

Content Item Descriptions

Row 1 | TID 300 specifies an "Equivalent Meaning of Concept Name" that allows the creating application to specify the preferred composed concept name representing the measurement and the associated post-coordination Concept Modifiers (e.g., the ASE terminology described in Section N.3 “Illustrative Mapping to ASE Concepts” in PS3.17 ).

Prev | Up | Next
TID 5202 Echo Section | Home | TID 5204 Wall Motion Analysis

DICOM PS3.16 2019a - Content Mapping Resource