DICOM PS3.17 2019a - Explanatory Information

XXX.3.10.3 Encoding Details (Current)
Prev | XXX.3.10 Highlighting Areas of Interest in Volume Rendered View | Next

#### XXX.3.10.3 Encoding Details

##### XXX.3.10.3.1 Volume Presentation State Relationship Module Recommendations

Table XXX.3.10.3.1-1. Volume Presentation State Relationship Module Recommendations

Attribute Name | Tag | Comment
Volumetric Presentation Input Set Sequence | (0070,120A) |
Item #1
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID1
>Presentation Input Type | (0070,1202) | Set to VOLUME
>Referenced Image Sequence | (0008,1140) | Reference to CT volume
Volumetric Presentation State Input Sequence | (0070,1201) |
Item #1
>Volumetric Presentation Input Number | (0070,1207) | Set to 1
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID1, referencing the first item in the Volumetric Presentation Input Set Sequence (0070,120A)
>Include VOI LUT Macro Table C.11-2B | Set to identity
>Crop | (0070,1204) | Set to NO

Prev | Up | Next
XXX.3.10.2 Encoding Outline | Home | XXX.3.10.3.2 Volume Render Geometry Module Recommendations

DICOM PS3.17 2019a - Explanatory Information