DICOM PS3.7 2019a - Message Exchange

C.5.16 No Such Argument (Current)
Prev | C.5 Failure Status Class | Next

### C.5.16 No Such Argument

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Affected SOP Class UID | (0000,0002) | UI | 1 | This optional field shall optionally contain the SOP Class UID for which the argument does not exist.
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0114H.
Event Type ID | (0000,1002) | US | 1 | This optional field contains the ID of the Event Type for which the argument does not exist. Permitted only in the N-EVENT-REPORT-RSP.
Action Type ID | (0000,1008) | US | 1 | This optional field contains the ID of the Action Type for which the argument does not exist. Permitted only in the N-ACTION-RSP.

Prev | Up | Next
C.5.15 Mistyped Argument | Home | C.5.17 No Such Attribute

DICOM PS3.7 2019a - Message Exchange