DICOM PS3.3 2019a - Information Object Definitions

C.8.8.14.14 Effective Wedge Angle (Current)
Prev | C.8.8.14 RT Beams Module | Next

##### C.8.8.14.14 Effective Wedge Angle

The Effective Wedge Angle (300A,00DE) describes the dosimetric angle of a motorized wedge accounting for the partial presence of the wedge in the beam. The presence of the wedge in the beam is specified by the Wedge Position (300A,0118) in the Wedge Position Sequence (300A,0116) included in the Control Point Sequence (300A,0111) of the current beam. When the wedge is in the beam throughout all control points, the Effective Wedge Angle will have the same value as the Wedge Angle (300A,00D5). Otherwise the Effective Wedge Angle will have a lower value than the Wedge Angle.

Prev | Up | Next
C.8.8.14.13 Angular Values in RT Beams Module | Home | C.8.8.14.15 Source to External Contour Distance and External Contour Entry Point

DICOM PS3.3 2019a - Information Object Definitions