DICOM PS3.7 2019a - Message Exchange

C.5.21 Processing Failure (Current)
Prev | C.5 Failure Status Class | Next

### C.5.21 Processing Failure

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Affected SOP Class UID | (0000,0002) | UI | 1 | This optional field contains the SOP Class UID on which the processing failure occurred.
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0110H.
Error Comment | (0000,0902) | LO | 1 | This optional field contains an application-specific text description of the error detected.
Error ID | (0000,0903) | US | 1 | This optional field contains an application-specific error code.
Affected SOP Instance UID | (0000,1000) | UI | 1 | This optional field shall optionally contain the UID of the SOP Instance on which the processing failure occurred.

Prev | Up | Next
C.5.20 No Such SOP Class | Home | C.5.22 Resource Limitation

DICOM PS3.7 2019a - Message Exchange