DICOM PS3.4 2019a - Service Class Specifications

H.4.3.2.3 SOP Class Definition and UID (Current)
Prev | H.4.3.2 Basic Color Image Box SOP Class | Next

##### H.4.3.2.3 SOP Class Definition and UID

The Basic Color Image Box SOP Class UID shall have the value "1.2.840.10008.5.1.1.4.1".

Prev | Up | Next
H.4.3.2.2 DIMSE Service Group | Home | H.4.3.3 Referenced Image Box SOP Class (Retired)

DICOM PS3.4 2019a - Service Class Specifications