DICOM PS3.7 2019b - Message Exchange

7.3 Service Modes (Current)
Prev | 7 Service Overview | Next

## 7.3 Service Modes

Operations and notifications, on an Association, are used in one of the following two modes:

1. synchronous

2. asynchronous

In the synchronous mode, the invoking DIMSE Service User, on an established Association, requires a response from the performing DIMSE Service User before invoking another operation or notification.

In the asynchronous mode, the invoking DIMSE Service User, on an established Association, may continue to invoke further operations or notifications to the performing DIMSE Service User without awaiting a response. In the asynchronous mode, the performing DIMSE Service User may respond to the operations or notifications in a different order than they were received.

The mode selection (synchronous or asynchronous) is determined at Association establishment time. The synchronous mode serves as the default mode and shall be supported by all DIMSE Service Users. The asynchronous mode is optional and the maximum number of outstanding operations/notifications is negotiated during Association establishment. This negotiation is accomplished by Application Association Information as defined in Annex D.

Prev | Up | Next
7.2 DIMSE Service User Interaction | Home | 7.4 Association Services

DICOM PS3.7 2019b - Message Exchange