DICOM PS3.3 2019b - Information Object Definitions

C.8.19.6.5 X-Ray Frame Detector Parameters Macro (Current)
Prev | C.8.19.6 Enhanced XA/XRF Image Functional Group Macros | Next

##### C.8.19.6.5 X-Ray Frame Detector Parameters Macro

Table C.8.19.6-5 specifies the Attributes containing the X-Ray Frame Detector Parameters Functional Group Macro.

Table C.8.19.6-5. X-Ray Frame Detector Parameters Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Frame Detector Parameters Sequence | (0018,9451) | 1 | Sequence containing the detector properties for this frame. Only a single Item shall be included in this Sequence.
>Detector Active Time | (0018,7014) | 3 | Time in mSec that the detector is active during acquisition of this image. ### Note This activation window overlaps the time of the X-Ray exposure as defined by Exposure Time in ms (0018,9328) and Detector Activation Offset From Exposure (0018,7016).
>Detector Activation Offset From Exposure | (0018,7016) | 3 | Offset time in mSec that the detector becomes active after the X-Ray beam is turned on during acquisition of this image. May be negative.

Prev | Up | Next
C.8.19.6.4 X-Ray Frame Pixel Data Properties Macro | Home | C.8.19.6.6 X-Ray Calibration Device Usage Macro

DICOM PS3.3 2019b - Information Object Definitions