DICOM PS3.3 2019b - Information Object Definitions

C.11.23.2 Input Sequence Position Index (Current)
Prev | C.11.23 Volumetric Presentation State Relationship Module | Next

#### C.11.23.2 Input Sequence Position Index

A sequence of inputs may be used in an animation. In this form of animation, the Presentation State is applied to each input in a sequence of inputs to produce a moving view. The inputs belonging to the input sequence are identified by the inclusion of an Input Sequence Position Index (0070,1203) value for each included input. See the INPUT_SEQ animation style in Section C.11.29.

### Note

Examples include:

- a sequence of cardiac volume acquisitions acquired through a heart cycle

- a sequence of volume acquisitions during multiple phases of passage of a contrast agent

There is another animation method "Presentation Sequence Animation" that may be used. See Section C.11.22.2 “Presentation Sequence Collection UID”.

Prev | Up | Next
C.11.23 Volumetric Presentation State Relationship Module | Home | C.11.23.3 Volumetric Presentation State Reference Coordinate System

DICOM PS3.3 2019b - Information Object Definitions