DICOM PS3.3 2019b - Information Object Definitions

A.75.3 Parametric Map IOD Module Table (Current)
Prev | A.75 Parametric Map IOD | Next

### A.75.3 Parametric Map IOD Module Table

Table A.75-1. Parametric Map IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Parametric Map Series | C.8.32.1 | M
Clinical Trial Series | C.7.3.2 | U
Frame of Reference | Frame of Reference | C.7.4.1 | M
Equipment | General Equipment | C.7.5.1 | M
Enhanced General Equipment | C.7.5.2 | M
Image | General Image | C.7.6.1 | M
General Reference | C.12.4 | U
Image Pixel | C.7.6.3 | C - Required if integer pixels
Floating Point Image Pixel | C.7.6.24 | C - Required if 32 bit floating point pixels
Double Floating Point Image Pixel | C.7.6.25 | C - Required if 64 bit floating point pixels
Parametric Map Image | C.8.32.2 | M
Multi-frame Functional Groups | C.7.6.16 | M
Multi-frame Dimension | C.7.6.17 | M
Palette Color Lookup Table | C.7.9 | C - Required if Pixel Presentation (0008,9205) in the Parametric Map image Module equals COLOR_RANGE and Palette Color Lookup Table UID (0028,1199) is not present.
Cardiac Synchronization | C.7.6.18.1 | U
Respiratory Synchronization | C.7.6.18.2 | U
Bulk Motion Synchronization | C.7.6.18.3 | U
Acquisition Context | C.7.6.14 | M
Device | C.7.6.12 | U
Specimen | C.7.6.22 | U
Common Instance Reference | C.12.2 | C - Required if Referenced Image Functional Group (Section C.7.6.16.2.5) or Derivation Image Functional Group (Section C.7.6.16.2.6) is present.
SOP Common | C.12.1 | M
Frame Extraction | C.12.3 | C - Required if the SOP Instance was created in response to a Frame-Level retrieve request

Prev | Up | Next
A.75.2 Parametric Map IOD Entity-Relationship Model | Home | A.75.4 Parametric Map IOD Content Constraints

DICOM PS3.3 2019b - Information Object Definitions