DICOM PS3.3 2019b - Information Object Definitions

C.11.8 Softcopy VOI LUT Module (Current)
Prev | C.11 Look Up Tables and Presentation States | Next

### C.11.8 Softcopy VOI LUT Module

Table C.11.8-1 specifies the Attributes that describe the Softcopy VOI LUT. These Attributes have the same meaning and behavior as defined in the Section C.11.2 VOI LUT Module.

Table C.11.8-1. Softcopy VOI LUT Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Softcopy VOI LUT Sequence | (0028,3110) | 1 | Defines a Sequence of VOI LUTs or Window Centers and Widths and to which images and frames they apply. No more than one VOI LUT Sequence containing a single Item or one pair of Window Center/Width values shall be specified for each image or frame. One or more Items shall be included in this Sequence.
>Referenced Image Sequence | (0008,1140) | 1C | The subset of images and frames listed in the Presentation State Relationship Module, to which this VOI LUT or Window Center and Width applies. One or more Items shall be included in this Sequence. Required if the VOI LUT transformation in this Item does not apply to all the images and frames listed in the Presentation State Relationship Module.
>>Include Table 10-3 “Image SOP Instance Reference Macro Attributes” |
>Include Table C.11-2b “VOI LUT Macro Attributes” |

Prev | Up | Next
C.11.7 Overlay Activation Module | Home | C.11.9 Presentation Series Module

DICOM PS3.3 2019b - Information Object Definitions