DICOM PS3.8 2019b - Network Communication Support for Message Exchange

9.3.8 A-ABORT PDU Structure (Current)
Prev | 9.3 DICOM Upper Layer Protocol for TCP/IP Data Units Structure | Next

### 9.3.8 A-ABORT PDU Structure

An A-ABORT PDU shall be made of a sequence of mandatory fields. Table 9-26 shows the sequence of the fields.

The A-ABORT PDU shall support both the A-ABORT Service (user initiated) and the A-P-ABORT Service (provider initiated).

Table 9-26. A-ABORT PDU Fields

PDU bytes | Field name | Description of field
--- | --- | ---
1 | PDU-type | 07H
2 | Reserved | This reserved field shall be sent with a value 00H but not tested to this value when received.
3-6 | PDU-length | This PDU-length shall be the number of bytes from the first byte of the following field to the last byte of the Reserved field. In the case of this PDU, it shall have the fixed value of 00000004H encoded as an unsigned binary number.
7 | Reserved | This reserved field shall be sent with a value 00H but not tested to this value when received.
8 | Reserved | This reserved field shall be sent with a value 00H but not tested to this value when received.
9 | Source | This Source field shall contain an integer value encoded as an unsigned binary number. One of the following values shall be used: 0 - DICOM UL service-user (initiated abort) 1 - reserved 2 - DICOM UL service-provider (initiated abort)
10 | Reason/Diag., | This field shall contain an integer value encoded as an unsigned binary number. If the Source field has the value (2) "DICOM UL service-provider", it shall take one of the following: 0 - reason-not-specified1 - unrecognized-PDU 2 - unexpected-PDU 3 - reserved 4 - unrecognized-PDU parameter 5 - unexpected-PDU parameter 6 - invalid-PDU-parameter value If the Source field has the value (0) "DICOM UL service-user", this reason field shall not be significant. It shall be sent with a value 00H but not tested to this value when received. ### Note The reserved fields are used to preserve symmetry with OSI ACSE/Presentation Services and Protocol.

Prev | Up | Next
9.3.7 A-RELEASE-RP PDU Structure | Home | 10 Conformance

DICOM PS3.8 2019b - Network Communication Support for Message Exchange