DICOM PS3.3 2019b - Information Object Definitions

A.33.4 Blending Softcopy Presentation State IOD (Current)
Prev | A.33 Softcopy Presentation State Information Object Definitions | Next

### A.33.4 Blending Softcopy Presentation State IOD

#### A.33.4.1 Blending Softcopy Presentation State IOD Description

The Blending Softcopy Presentation State Information Object Definition (IOD) specifies information that may be used to blend two sets of images that are referenced from within the IOD for the purpose of presentation (display).

It includes capabilities for specifying:

1. the output color space in PCS-Values

2. grayscale contrast transformations including modality and VOI LUT for both the underlying and superimposed image sets

3. a color palette to map the transformed grayscale values of the superimposed image set into pseudo-color

4. selection of the area of the blended images to display and whether to rotate or flip it

5. image and display relative annotations, including graphics, text and overlays

### Note

This IOD does not support presentation control for a set of images for which the modality LUT varies on a frame-by-frame basis. Other Presentation State IODs (standard or private) may support such images.

Prev | Up | Next
A.33.3.3 Pseudo-color Softcopy Presentation State IOD Module Table | Home | A.33.4.2 Blending Softcopy Presentation State IOD Entity-Relationship Model

DICOM PS3.3 2019b - Information Object Definitions