DICOM PS3.2 2019b - Conformance

E.4.4.2 Parameters (Current)
Prev | E.4.4 Configuration | Next

### E.4.4.2 Parameters

A large number of parameters related to Print Management, Communications and general operation can be configured using the Service/Installation Tool. The following table shows those configuration parameters relevant to DICOM communication. See the EXAMPLE-PRINT-SERVER-MANAGEMENT Configuration Service Manual for details on general configuration capabilities.

Table E.4.4-2. Configuration Parameters Table

Parameter | Configurable (Yes/No) | Default Value
--- | --- | ---
General Parameters
Max PDU Receive Size | Yes | 128 KB
Max PDU Send Size(If the receiver supports a smaller Max PDU Receive Size then the Max PDU Send Size will be reduced accordingly for the duration of the Association. Max PDU Receive Size information is exchanged during DICOM Association Negotiation in the Maximum Length Sub-Item of the A-ASSOCIATION-RQ and A-ASSOCIATE-AC) | Yes | 128 KB
Time-out waiting for a acceptance or rejection response to an Association Request (Application level Timeout). | Yes | 20 s
Time-out waiting for a response to an Association release request (Application level Timeout) | Yes | 30 s
Time-out waiting for completion of a TCP/IP connect request (Low-level timeout) | Yes | 20 s
Time-out awaiting a Response to a DIMSE Request (Low level Timeout) | Yes | 360 s
Time-out for waiting for data between TCP/IP-packets (Low level Timeout) | Yes | 30 s
Maximum number of simultaneous Associations | Yes | 8
Supported Transfer Syntaxes | Yes | Implicit VR Little Endian Explicit VR Little Endian
Print Server Management
Default Print parameters: Max density, Min Density, Contrast, Border Density, Trim, Magnification type, Smoothing factor, Polarity, Number of Copies, Cropping Algorithm, Orientation. | Yes | Configurable
Number of times a failed print-job may be retried | Yes | 3
Delay between retrying failed print-jobs | Yes | 60s
Printer Bit-depth Configurable: 8 or 12 | Yes | 12
Custom Format | No | NA
Media Type: Transparent (Film), Reflective (Paper) | Yes | Transparent
Media size Configurable: 8IN X 10IN 11IN X 14IN 14IN X 14IN 14IN X 17IN | Yes | 14IN X 17IN
Maximum number of printable pixel matrix per supported Media size; see Note | No | 8x10 - 2286x2836 11x14 - 4096x3195 14x14 - 4096x4108 14x17 - 4096x5120
Maximum number of collated films in a film session | Yes | 12
Support N-EVENT-REPORT (On/Off for either Printer, Print Job or both). | Yes | On
Handling of print jobs when requested Media Type and/or Film Size are not currently installed. The options are: Queue the print job until the film matching the requested Media Type and/or Film Size is loaded. Print on the film currently loaded in the printer. | Yes | Print on available media
Print SCP time-out waiting for a SCU confirmation to a Print Status N-EVENT-REPORT | Yes | 60 s
Print SCP time-out waiting for a SCU confirmation to a Print Job N-EVENT-REPORT | Yes | 60 s
Supported Transfer Syntaxes (separately configurable for each remote SCU printer) | Yes | Implicit VR Little Endian Explicit VR Little Endian

### Note

The adjustment (Magnification or Clipping) of the original image to the Printable image size is described in the Printer Service Manual.

Prev | Up | Next
E.4.4 Configuration | Home | E.5 Media Interchange

DICOM PS3.2 2019b - Conformance