DICOM PS3.8 2019b - Network Communication Support for Message Exchange

9.3.4 A-ASSOCIATE-RJ PDU Structure (Current)
Prev | 9.3 DICOM Upper Layer Protocol for TCP/IP Data Units Structure | Next

### 9.3.4 A-ASSOCIATE-RJ PDU Structure

An A-ASSOCIATE-RJ PDU shall be made of a sequence of mandatory fields. Table 9-21 shows the sequence of the mandatory fields.

Table 9-21. ASSOCIATE-RJ PDU Fields

PDU bytes | Field name | Description of field
--- | --- | ---
1 | PDU-type | 03H
2 | Reserved | This reserved field shall be sent with a value 00H but not tested to this value when received.
3-6 | PDU-length | This PDU-length shall be the number of bytes from the first byte of the following field to the last byte of the Reason/Diag. field. In the case of this PDU, it shall have the fixed value of 00000004H encoded as an unsigned binary number.
7 | Reserved | This reserved field shall be sent with a value 00H but not tested to this value when received.
8 | Result | This Result field shall contain an integer value encoded as an unsigned binary number. One of the following values shall be used: 1 - rejected-permanent 2 - rejected-transient
9 | Source | This Source field shall contain an integer value encoded as an unsigned binary number. One of the following values shall be used: 1 - DICOM UL service-user 2 - DICOM UL service-provider (ACSE related function) 3 - DICOM UL service-provider (Presentation related function)
10 | Reason/Diag. | This field shall contain an integer value encoded as an unsigned binary number. If the Source field has the value (1) "DICOM UL service-user", it shall take one of the following: 1 - no-reason-given 2 - application-context-name-not-supported 3 - calling-AE-title-not-recognized 4-6 - reserved 7 - called-AE-title-not-recognized 8-10 - reserved If the Source field has the value (2) "DICOM UL service provided (ACSE related function)", it shall take one of the following: 1 - no-reason-given 2 - protocol-version-not-supported If the Source field has the value (3) "DICOM UL service provided (Presentation related function)", it shall take one of the following: 0 - reserved 1 - temporary-congestio 2 - local-limit-exceeded 3-7 - reserved ### Note The reserved fields are used to preserve symmetry with OSI ACSE/Presentation Services and Protocols.

Prev | Up | Next
9.3.3.3 User Information Item Structure | Home | 9.3.5 P-DATA-TF PDU Structure

DICOM PS3.8 2019b - Network Communication Support for Message Exchange