DICOM PS3.16 2019b - Content Mapping Resource

TID 3309 Stress Echo Measurement Group (Current)
Prev | Stress Testing Report Templates | Next

### TID 3309 Stress Echo Measurement Group

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3309. Stress Echo Measurement Group

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | DT (121070, DCM, "Findings") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (121058, DCM, "Procedure reported") | 1 | M |  | DT (40701008, SCT, "Echocardiography")
3 | > | CONTAINS | INCLUDE | DTID 5203 “Echo Measurement” | 1-n | U |  | $Measurement = DCID 12200 “Echocardiography Left Ventricle” $Method = CID 12227 “Echocardiography Measurement Method”
4 | >> | HAS CONCEPT MOD | CODE | EV (363698007, SCT, "Finding Site") | 1 | MC | IF Row 3 measurement concept is in CID 12222 “Orifice Flow Properties” | EV (87878005, SCT, "Left Ventricle")
5 | > | CONTAINS | INCLUDE | DTID 5203 “Echo Measurement” | 1-n | U |  | $Measurement = DCID 12211 “Echocardiography Aortic Valve” $Method = CID 12227 “Echocardiography Measurement Method”
6 | >> | HAS CONCEPT MOD | CODE | EV (363698007, SCT, "Finding Site") | 1 | MC | IF Row 5 measurement concept is in CID 12222 “Orifice Flow Properties” | EV (34202007, SCT, "Aortic Valve")
7 | > | CONTAINS | INCLUDE | DTID 5203 “Echo Measurement” | 1-n | U |  | $Measurement = DCID 12207 “Echocardiography Mitral Valve” $Method = CID 12227 “Echocardiography Measurement Method”
8 | >> | HAS CONCEPT MOD | CODE | EV (363698007, SCT, "Finding Site") | 1 | MC | IF Row 7 measurement concept is in CID 12222 “Orifice Flow Properties” | EV (91134007, SCT, "Mitral Valve")
9 | > | CONTAINS | INCLUDE | DTID 5203 “Echo Measurement” | 1-n | U |  | $Measurement = DCID 12208 “Echocardiography Tricuspid Valve” $Method = CID 12227 “Echocardiography Measurement Method”
10 | >> | HAS CONCEPT MOD | CODE | EV (363698007, SCT, "Finding Site") | 1 | MC | IF Row 9 measurement concept is in CID 12222 “Orifice Flow Properties” | EV (46030003, SCT, "Tricuspid Valve")
11 | > | CONTAINS | INCLUDE | DTID 5204 “Wall Motion Analysis” | 1 | U |  | $Procedure = DT (35757004, SCT, "Echocardiography for Determining Ventricular Contraction")

Content Item Descriptions

Rows 3-10 | These invocations of TID 5203 “Echo Measurement” do not include an inherited Findings Site concept, for example as in the invocations of TID 5203 “Echo Measurement” from TID 5202 “Echo Section”. Echo measurements that do not have the associated Finding Site pre-coordinated in the measurement concept (i.e., the orifice flow measurements of CID 12222 “Orifice Flow Properties”), shall have the Finding Site explicitly post-coordinated with a Concept Modifier (Rows 4, 6, 8, and 10). This Template does not include the concept of an Image Library, for example as used in TID 5200 “Echocardiography Procedure Report”. Image Content Items in the Echo Measurement Template shall be included with by-value relationships, not with by-reference relationships.

Prev | Up | Next
TID 3307 NM/PET Perfusion Measurement Group | Home | TID 3311 Stress Test Summary

DICOM PS3.16 2019b - Content Mapping Resource