DICOM PS3.16 2019b - Content Mapping Resource

TID 10003A Irradiation Event X-Ray Detector Data (Current)
Prev | X-Ray Radiation Dose SR IOD Templates | Next

### TID 10003A Irradiation Event X-Ray Detector Data

This Template contains data that is expected to be available to the X-Ray detector or plate reader component of the equipment.

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 10003A. Irradiation Event X-Ray Detector Data

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | NUM | EV (113845, DCM, "Exposure Index") | 1 | MC | IF the value is displayable to the X-Ray system operator. | UNITS = EV (1, UCUM, "no units")
2 |  |  | NUM | EV (113846, DCM, "Target Exposure Index") | 1 | MC | IF the value is displayable to the X-Ray system operator. | UNITS = EV (1, UCUM, "no units")
3 |  |  | NUM | EV (113847, DCM, "Deviation Index") | 1 | MC | IF the value is displayable to the X-Ray system operator. | UNITS = EV (1, UCUM, "no units")
4 |  |  | INCLUDE | DTID 1021 “Device Participant” | 1 | U |  | $DeviceProcedureRole = EV (113942, DCM, "X-Ray Reading Device")
5 |  |  | IMAGE | EV (113795, DCM, "Acquired Image") | 1-n | MC | IFF Image Object is created for this irradiation event |

Content Item Descriptions

Row 4 | The device that read the detector of this Irradiation Event. E.g., the CR Plate Reader.
Row 5 | Reference to Image instances created during this event, if any. The UID reference(s) provided here shall be the values at the time the images were initially created. (Note that image UIDs may be changed as the images are managed over a long term.)

Prev | Up | Next
TID 10003 Irradiation Event X-Ray Data | Home | TID 10003B Irradiation Event X-Ray Source Data

DICOM PS3.16 2019b - Content Mapping Resource