DICOM PS3.7 2019b - Message Exchange

9.3.4.2 C-MOVE-RSP (Current)
Prev | 9.3.4 C-MOVE Protocol | Next

#### 9.3.4.2 C-MOVE-RSP

The C-MOVE-RSP Message contains fields as defined in Table 9.3-10 and in Annex C. Each field shall conform to DICOM encoding and Value Representation as defined in PS3.5. Fields are required as specified in the C-MOVE service definition unless otherwise noted in Table 9.3-10. Fields not specified in the C-MOVE service definition but present in Table 9.3-10 are required by the DIMSE-C protocol.

Table 9.3-10. C-MOVE-RSP Message Fields

Message Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Command Group Length | (0000,0000) | UL | 1 | The even number of bytes from the end of the value field to the beginning of the next group.
Affected SOP Class UID | (0000,0002) | UI | 1 | SOP Class UID associated with the operation.
Command Field | (0000,0100) | US | 1 | This field distinguishes the DIMSE-C operation conveyed by this Message. The value of this field shall be set to 8021H for the C-MOVE-RSP Message.
Message ID Being Responded To | (0000,0120) | US | 1 | Shall be set to the value of the Message ID (0000,0110) field used in associated C-MOVE Message.
Command Data Set Type | (0000,0800) | US | 1 | This field indicates if a Data Set is present in the Message. This field shall be set to the value of 0101H (Null) if no Data Set is present; any other value indicates a Data Set is included in the Message.
Status | (0000,0900) | US | 1 | The value of this field depends upon the status type. Annex C defines the encoding of the status types defined in the service definition.
Number of Remaining Sub-operations | (0000,1020) | US | 1 | The number of remaining sub-operations to be invoked for this C-MOVE operation.
Number of Completed Sub-operations | (0000,1021) | US | 1 | The number of C-STORE sub-operations invoked by this C-MOVE operation that have completed successfully.
Number of Failed Sub-operations | (0000,1022) | US | 1 | The number of C-STORE sub-operations invoked by this C-MOVE operation that have failed.
Number of Warning Sub-operations | (0000,1023) | US | 1 | The number of C-STORE sub-operations invoked by this C-MOVE operation that generated warning responses.
Identifier | (no tag) | - | - | A Data Set that encodes attributes providing status information about the C-MOVE operation. See Section 9.1.4.1.6.

Prev | Up | Next
9.3.4 C-MOVE Protocol | Home | 9.3.4.3 C-CANCEL-MOVE-RQ

DICOM PS3.7 2019b - Message Exchange