DICOM PS3.3 2019b - Information Object Definitions

A.32.5.2 Video Endoscopic Image IOD Entity-Relationship Model (Current)
Prev | A.32.5 Video Endoscopic Image IOD | Next

#### A.32.5.2 Video Endoscopic Image IOD Entity-Relationship Model

This IOD uses the E-R Model in Section A.1.2, with only the Image IE below the Series IE. The Frame of Reference IE is not a component of this IOD.

### Note

1. The video may include audio channel(s) for acquiring Patient voice or physiological sounds, healthcare professionals' commentary, or environmental sounds.

2. The Frame Pointers Module has not been included because the selection of relevant sub-sequence(s) is usually made in a second workflow step and stored into separate Key Object Selection Documents.

3. The Curve entity was previously include in the list of entities that are not used, but has been retired from DICOM. It is still not used in this IOD. See PS3.3-2004.

Table A.32.5-1. Video Endoscopic Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Equipment | General Equipment | C.7.5.1 | M
Image | General Image | C.7.6.1 | M
General Reference | C.12.4 | U
Cine | C.7.6.5 | M
Multi-frame | C.7.6.6 | M
Image Pixel | C.7.6.3 | M
Acquisition Context | C.7.6.14 | M
Device | C.7.6.12 | U
Specimen | C.7.6.22 | C - Required if the Imaging Subject is a Specimen
VL Image | C.8.12.1 | M
ICC Profile | C.11.15 | U
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U
Frame Extraction | C.12.3 | C - Required if the SOP Instance was created in response to a Frame-Level retrieve request

Prev | Up | Next
A.32.5 Video Endoscopic Image IOD | Home | A.32.5.3 Video Endoscopic Image IOD Content Constraints

DICOM PS3.3 2019b - Information Object Definitions