DICOM PS3.3 2019b - Information Object Definitions

A.32 Visible Light Image Information Object Definitions (Current)
Prev | A Composite Information Object Definitions (Normative) | Next

## A.32 Visible Light Image Information Object Definitions

The Visible Light (VL) Image Information Object Definition (IOD) specifies images that are acquired by means of a camera or other sensors that are sensitive to visible or near-visible light.

Examples of types of equipment that create Visible Light Images include:

1. Rigid and flexible endoscopy equipment

2. Operation microscopes / colposcopes

3. Ophthalmology equipment

4. Digital or Video Cameras

5. Analysis microscopes

Separate IODs have been defined for specialized applications. Some support only single-frame images, some support both single-frame and multi-frame video images.

### A.32.1 VL Endoscopic Image IOD

#### A.32.1.1 VL Endoscopic Image IOD Description

The VL Endoscopic Image IOD specifies the Attributes of Single-frame VL Endoscopic Images.

#### A.32.1.2 VL Endoscopic Image IOD Entity-Relationship Model

This IOD uses the E-R Model in Section A.1.2, with only the Image IE below the Series IE. The Frame of Reference IE is not a component of this IOD.

### Note

1. An endoscopic procedure might include multiple Series of single-frame endoscopic images as well as one or more additional Series of related diagnostic images. The procedure might involve multiple Performed Procedure Steps, multiple endoscopes, and multiple anatomic regions and might be supervised, performed, and/or interpreted by one or more individuals.

2. Several distinct diagnostic or therapeutic processes might occur during an endoscopic procedure. For example: Endoscopic examination of duodenal mucosa, biopsy, lavage, or biliary stone removal.

3. The Curve entity was previously include in the list of entities that are not used, but has been retired from DICOM. It is still not used in this IOD. See PS3.3-2004.

Table A.32.1-1. VL Endoscopic Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Equipment | General Equipment | C.7.5.1 | M
Image | General Image | C.7.6.1 | M
General Reference | C.12.4 | U
Image Pixel | C.7.6.3 | M
Acquisition Context | C.7.6.14 | M
Device | C.7.6.12 | U
Specimen | C.7.6.22 | U
VL Image | C.8.12.1 | M
Overlay Plane | C.9.2 | U
ICC Profile | C.11.15 | U
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U

#### A.32.1.3 VL Endoscopic Image IOD Content Constraints

##### A.32.1.3.1 Modality

The value of Modality (0008,0060) shall be ES.

Prev | Up | Next
A.31.3 RT Treatment Summary Record IOD Module Table | Home | A.32.2 VL Microscopic Image IOD

DICOM PS3.3 2019b - Information Object Definitions