DICOM PS3.4 2019b - Service Class Specifications

S.3.2.4.3 Service Class Provider (Current)
Prev | S.3.2.4 Get Media Creation Result | Next

##### S.3.2.4.3 Service Class Provider

This operation allows the SCU to request from the SCP, selected Attribute Values for a specific Media Creation Management SOP Instance. This operation shall be invoked through the use of the DIMSE N-GET Service used in conjunction with the appropriate Media Creation Management SOP Instance.

The SCP shall return, via the N-GET response primitive, the N-GET Response Status Code applicable to the associated request. Contingent on the N-GET Response Status, the SCP shall return, via the N-GET Response Primitive, Attribute Values for all requested Attributes maintained by the SCP (see Table S.3.2.4.1-1). The SCP shall not return Data Elements for optional Attributes that are not maintained by the SCP.

The SCP shall return the entire content of a Sequence if a Sequence Attribute is requested.

Prev | Up | Next
S.3.2.4.2 Service Class User | Home | S.3.2.4.4 Status Codes

DICOM PS3.4 2019b - Service Class Specifications