DICOM PS3.3 2019b - Information Object Definitions

C.8.8.14.7 Cumulative Dose Reference Coefficient (Current)
Prev | C.8.8.14 RT Beams Module | Next

##### C.8.8.14.7 Cumulative Dose Reference Coefficient

The Cumulative Dose Reference Coefficient (300A,010C) is the value by which Beam Dose (300A,0084) is multiplied to obtain the dose to the referenced dose reference site at the current control point (and after previous control points have been successfully administered). The Cumulative Dose Reference Coefficient (300A,010C) is by definition zero for the initial control point. The Cumulative Dose Reference Coefficient (300A,010C) of the final control point multiplied by Beam Dose (300A,0084) results in the final dose to the referenced dose reference site for the current beam. Dose calculation for dose reference sites other than points is not well defined.

Prev | Up | Next
C.8.8.14.6 Absolute and Relative Machine Coordinates | Home | C.8.8.14.8 Machine Rotations

DICOM PS3.3 2019b - Information Object Definitions