DICOM PS3.4 2019c - Service Class Specifications

R.2 Conformance Overview (Current)
Prev | R Instance Availability Notification Service Class (Normative) | Next

## R.2 Conformance Overview

The Instance Availability Notification Service Class consists of a single SOP Class: the Instance Availability Notification SOP Class.

The SOP Class specifies Attributes, operations, and behavior applicable to the SOP Class. The conformance requirements shall be specified in terms of the Service Class Provider (SCP) and the Service Class User (SCU).

The Instance Availability Notification Service Class uses the Instance Availability Notification IOD as defined in PS3.3 and the N-CREATE DIMSE Service specified in PS3.7.

Prev | Up | Next
R Instance Availability Notification Service Class (Normative) | Home | R.3 Instance Availability Notification SOP Class

DICOM PS3.4 2019c - Service Class Specifications