DICOM PS3.17 2019c - Explanatory Information

XXX.3.11.3.4 Render Display Module Recommendations (Current)
Prev | XXX.3.11.3 Encoding Details | Next

##### XXX.3.11.3.4 Render Display Module Recommendations

Table XXX.3.11.3.4-1. Render Display Module Recommendations

Attribute Name | Tag | Comment
Pixel Presentation | (0008, 9205) | Set to 'TRUE_COLOR'
Volume Stream Sequence | (0070,1A08) | One item in this sequence
Item #1 in Volume Stream Sequence
>Volumetric Presentation Input Set UID | (0070,1209) | UID1
>Presentation State Classification Component Sequence | (0070,1801) | Include three items, one for each classification component
>Item #1 in Presentation State Classification Component Sequence
>>Component Type | (0070, 1802) | Set to 'ONE_TO_RGBA'
>>Component Input Sequence | (0070, 1803) | Set only one item in this sequence, since the component has only one input.
>>Item #1 in Component Input Sequence
>>>Volumetric Presentation Input Index | (0070,1804) | Set to '1' for the bones.
>>RGB LUT Transfer Function | (0028,140F) | Set to 'TABLE'.
>>Alpha LUT Transfer Function | (0028,1410) | Set to 'TABLE'.
>> RGB Palette Color Lookup Table Descriptors and Data
>> Alpha Palette Color Lookup Table Descriptor and Data
>Item #2 in Presentation State Classification Component Sequence
>>Component Type | (0070, 1802) | Set to 'ONE_TO_RGBA'
>>Component Input Sequence | (0070, 1803) | Set only one item in this sequence, since the component has only one input.
>>Item #1 in Component Input Sequence
>>>Volumetric Presentation Input Index | (0070,1804) | Set to '2' for the segmented vessels and kidneys
>>RGB LUT Transfer Function | (0028,140F) | Set to 'TABLE'
>>Alpha LUT Transfer Function | (0028,1410) | Set to 'TABLE'.
>>RGB Palette Color Lookup Table Descriptors and Data
>>Alpha Palette Color Lookup Table Descriptor and Data
>Item #3 in Presentation State Classification Component Sequence
>>Component Type | (0070, 1802) | Set to 'ONE_TO_RGBA'
>>Component Input Sequence | (0070, 1803) | Set only one item in this sequence, since the component has only one input.
>>Item #1 in Component Input Sequence
>>Volumetric Presentation Input Index | (0070,1804) | Set to '3' for the segmented tumor.
>RGB LUT Transfer Function | (0028,140F) | Set to 'EQUAL_RGB'
>Alpha LUT Transfer Function | (0028,1410) | Set to "NONE".
Presentation State Compositor Component Sequence | (0070,1805) | empty
ICC Profile | (0028,2000) | Value corresponding to IEC 61966-2-1:1999
Color Space | (0028,2002) | Set to SRGB

Prev | Up | Next
XXX.3.11.3.3 Render Shading Module Recommendations | Home | XXX.3.12 Liver Resection Planning

DICOM PS3.17 2019c - Explanatory Information