DICOM PS3.3 2019c - Information Object Definitions

C.8.8.2.5 Single-Frame and Multi-frame Images (Current)
Prev | C.8.8.2 RT Image Module | Next

##### C.8.8.2.5 Single-Frame and Multi-frame Images

If the Multi-frame Module is present and the Cine Module is not present then the Frame Increment Pointer (0028,0009) shall have the Enumerated Value of 00200013 (Instance Number). If the Multi-frame Module and Cine Module are both present then the Frame Increment Pointer (0028,0009) shall have an Enumerated Value of either 00181063 (Frame Time) or 00181065 (Frame Time Vector).

Prev | Up | Next
C.8.8.2.4 Exposure Sequence | Home | C.8.8.2.6 Image Pixel Module Attributes

DICOM PS3.3 2019c - Information Object Definitions