DICOM PS3.2 2019c - Conformance

I.8.4 Grayscale Image Consistency (Current)
Prev | I.8 Annexes | Next

### I.8.4 Grayscale Image Consistency

The EXAMPLE-WADO-SERVICE assumes that the JPEG images will be displayed with monitors calibrated to the sRGB profile when rendering images.

Prev | Up | Next
I.8.3 Coded Terminology and Templates | Home | I.8.5 Standard Extended / Specialized / Private SOP Classes

DICOM PS3.2 2019c - Conformance