DICOM PS3.17 2019c - Explanatory Information

XXX.3.3.2 Encoding Outline (Current)
Prev | XXX.3.3 Replacing Set of Derived Images with Multiple Volumetric Presentation States | Next

#### XXX.3.3.2 Encoding Outline

For Planar MPR views that can be moved or rotated by the display application, no special encodings in the Planar MPR VPS SOP Instance are necessary.

Figure XXX.3.3-2. One Volumetric Presentations States is created for each of the MPR views. The VPS Instances have the same value of Presentation Display Collection UID (0070,1101)

In general, the individual VPS instances may have any orientation and be in any location.

Prev | Up | Next
XXX.3.3 Replacing Set of Derived Images with Multiple Volumetric Presentation States | Home | XXX.3.3.3 Encoding Details

DICOM PS3.17 2019c - Explanatory Information