DICOM PS3.3 2019c - Information Object Definitions

A.7.4 US Multi-frame Image IOD Module Table (Current)
Prev | A.7 Ultrasound Multi-frame Image IOD | Next

### A.7.4 US Multi-frame Image IOD Module Table

Table A.7-1 specifies the Modules of the US Multi-frame Image IOD.

Table A.7-1. US Multi-frame Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Frame of Reference | Frame of Reference | C.7.4.1 | U
Synchronization | C.7.4.2 | C - Required if Modality (0008,0060) = IVUS. May be present otherwise.
Equipment | General Equipment | C.7.5.1 | M
Image | General Image | C.7.6.1 | M
General Reference | C.12.4 | U
Image Pixel | C.7.6.3 | M
Contrast/Bolus | C.7.6.4 | C - Required if contrast media was used in this image.
Cine | C.7.6.5 | M
Multi-frame | C.7.6.6 | M
Frame Pointers | C.7.6.9 | U
Palette Color Lookup Table | C.7.9 | C - Required if Photometric Interpretation (0028,0004) has a value of PALETTE COLOR
Device | C.7.6.12 | U
Specimen | C.7.6.22 | U
US Region Calibration | C.8.5.5 | U
US Image | C.8.5.6 | M
VOI LUT | C.11.2 | U
ICC Profile | C.11.15 | U
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U
Frame Extraction | C.12.3 | C - Required if the SOP Instance was created in response to a Frame-Level retrieve request

### Note

1. For the purpose of conveying ultrasound protocol data management information it is recommended that the Performed Protocol Code Sequence (0040,0260) be assigned the code value(s) of the performed ultrasound protocol, if any. The Baseline Context Group for these code values is CID 12001 “Ultrasound Protocol Types” (defined in PS3.16).

2. The US Frame of Reference Module was previously included in this IOD, but has been retired. See PS3.3-2003.

#### A.7.4.1 Mutually Exclusive IEs

### Note

A Curve IE was previously included in this IOD that was mutually exclusive with the Image IE, but has been retired. See PS3.3-2004.

Prev | Up | Next
A.7.3 US Image IOD Module Table (Retired) | Home | A.8 Secondary Capture Image IOD

DICOM PS3.3 2019c - Information Object Definitions