DICOM PS3.3 2019c - Information Object Definitions

A.34.3 12-Lead Electrocardiogram IOD (Current)
Prev | A.34 Waveform Information Object Definitions | Next

### A.34.3 12-Lead Electrocardiogram IOD

#### A.34.3.1 12-Lead ECG IOD Description

The 12-Lead Electrocardiogram (12-Lead ECG) IOD is the specification of digitized electrical signals from the patient cardiac conduction system collected on the body surface, which has been acquired by an ECG modality or by an ECG acquisition function within an imaging modality.

Prev | Up | Next
A.34.2.4.5 Waveform Sample Interpretation | Home | A.34.3.2 12-Lead ECG IOD Entity-Relationship Model

DICOM PS3.3 2019c - Information Object Definitions