DICOM PS3.3 2019c - Information Object Definitions

A.64.4 RT Beams Delivery Instruction IOD Content Constraints (Current)
Prev | A.64 RT Beams Delivery Instruction IOD | Next

### A.64.4 RT Beams Delivery Instruction IOD Content Constraints

#### A.64.4.1 Modality

The value of modality (0008,0060) shall be PLAN.

Prev | Up | Next
A.64.3 RT Beams Delivery Instruction IOD Module Table | Home | A.65 Ophthalmic Visual Field Static Perimetry Measurements IOD

DICOM PS3.3 2019c - Information Object Definitions