DICOM PS3.17 2019e - Explanatory Information

V.5 Hanging Protocol Query Example (Current)
Prev | V Hanging Protocols (Informative) | Next

## V.5 Hanging Protocol Query Example

The following is an example of a general C-FIND Request for the Hanging Protocol Information Model - FIND SOP Class that is searching for all Chest related Hanging Protocols for the purpose of reading projection Chest X-ray. The user is at a workstation that has two 2Kx2.5K screens.

C-FIND Request:

Nesting | Attribute | Tag | VR | VL (hex) | Value
--- | --- | --- | --- | --- | ---
| Affected SOP Class UID | (0000,0002) | UI | 0018 | 1.2.840.10008.5.1.4.38.2
| Command Field | (0000,0100) | US | 0002 | 0020H [C-FIND-RQ]
| Message ID | (0000,0110) | US | 0002 | 0010H
| Priority | (0000,0700) | US | 0002 | 0000H [MEDIUM]
| Data Set Type | (0000,0800) | US | 0002 | 0102H
| SOP Class UID | (0008,0016) | UI | 0000 |
| SOP Instance UID | (0008,0018) | UI | 0000 |
| Hanging Protocol Name | (0072,0002) | SH | 0000 |
| Hanging Protocol Description | (0072,0004) | LO | 0000 |
| Hanging Protocol Level | (0072,0006) | CS | 0000 |
| Hanging Protocol Creator | (0072,0008) | LO | 0000 |
| Hanging Protocol Creation DateTime | (0072,000A) | DT | 0000 |
| Hanging Protocol Definition Sequence | (0072,000C) | SQ | ffffffff |
%item |  |  |  |  |
> | Modality | (0008,0060) | CS | 0000 |
> | Anatomic Region Sequence | (0008,2218) | SQ | ffffffff |
%item |  |  |  |  |
>> | Code Value | (0008,0100) | SH | 0008 | 51185008
>> | Coding Scheme Designator | (0008,0102) | SH | 0004 | SCT
>> | Code Meaning | (0008,0104) | LO | 0006 | Chest
%enditem |  |  |  |  |
%endseq |  |  |  |  |
> | Procedure Code Sequence | (0008,1032) | SQ | 0000 |
> | Laterality | (0020,0060) | CS | 0000 |
> | Reason for Requested Procedure Code Sequence | (0040,100A) | SQ | 0000 |
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Hanging Protocol User Identification Code Sequence | (0072,000E) | SQ | 0000 |
| Number of Priors Referenced | (0072,0014) | US | 0000 |
| Number of Screens | (0072,0100) | US | 0000 |
| Nominal Screen Definition Sequence | (0072,0102) | SQ | 0000 |

The following is an example of a set of C-FIND Responses for the Hanging Protocol Information Model - FIND SOP Class, answering the C-FIND Request listed above. There are a few matches for this general query. The application needs to select the best choice among the matches, which is the second response. The first response is for Chest CT, and the third response does not match the user's workstation environment as well as does the second.

C-FIND Response #1:

Nesting | Attribute | Tag | VR | VL (hex) | Value
--- | --- | --- | --- | --- | ---
| Affected SOP Class UID | (0000,0002) | UI | 0018 | 1.2.840.10008.5.1.4.38.2
| Command Field | (0000,0100) | US | 0002 | 8020H [C-FIND-RSP]
| Message ID Being Responded To | (0000,0120) | US | 0002 | 0010H
| Data Set Type | (0000,0800) | US | 0002 | 0102H
| Status | (0000,0900) | US | 0002 | FF00H [Pending]
| SOP Class UID | (0008,0016) | UI | 0018 | 1.2.840.10008.5.1.4.38.1
| SOP Instance UID | (0008,0018) | UI | 0024 | 1.2.840.10008.5.1.4.1.1.76392.999.2
| Hanging Protocol Name | (0072,0002) | SH | 000a | CT 1 prior
| Hanging Protocol Description | (0072,0004) | LO | 0038 | Dual screen layout for current and single prior chest CT
| Hanging Protocol Level | (0072,0006) | CS | 000c | SINGLE_USER
| Hanging Protocol Creator | (0072,0008) | LO | 0008 | Dr. Chan
| Hanging Protocol Creation DateTime | (0072,000A) | DT | 000c | 200408210718
| Hanging Protocol Definition Sequence | (0072,000C) | SQ | ffffffff |
%item |  |  |  |  |
> | Modality | (0008,0060) | CS | 0002 | CT
> | Anatomic Region Sequence | (0008,2218) | SQ | ffffffff |
%item |  |  |  |  |
>> | Code Value | (0008,0100) | SH | 0008 | 51185008
>> | Coding Scheme Designator | (0008,0102) | SH | 0004 | SCT
>> | Code Meaning | (0008,0104) | LO | 0006 | Chest
%enditem |  |  |  |  |
%endseq |  |  |  |  |
> | Procedure Code Sequence | (0008,1032) | SQ | 0000 |
> | Laterality | (0020,0060) | CS | 0000 |
> | Reason for Requested Procedure Code Sequence | (0040,100A) | SQ | 0000 |
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Hanging Protocol User Identification Code Sequence | (0072,000E) | SQ | 0000 |
%item |  |  |  |  |
> | Code Value | (0008,0100) | SH | 000a | 58489749P
> | Coding Scheme Designator | (0008,0102) | SH | 0008 | HOSP_ID
> | Code Meaning | (0008,0104) | LO | 000e | Susan H. Chan
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Number of Priors Referenced | (0072,0014) | US | 0002 | 1
| Number of Screens | (0072,0100) | US | 0002 | 2
| Nominal Screen Definition Sequence | (0072,0102) | SQ | 0000 |

C-FIND Response #2:

Nesting | Attribute | Tag | VR | VL (hex) | Value
--- | --- | --- | --- | --- | ---
| Affected SOP Class UID | (0000,0002) | UI | 0018 | 1.2.840.10008.5.1.4.38.2
| Command Field | (0000,0100) | US | 0002 | 8020H [C-FIND-RSP]
| Message ID Being Responded To | (0000,0120) | US | 0002 | 0010H
| Data Set Type | (0000,0800) | US | 0002 | 0102H
| Status | (0000,0900) | US | 0002 | FF00H [Pending]
| SOP Class UID | (0008,0016) | UI | 0018 | 1.2.840.10008.5.1.4.38.1
| SOP Instance UID | (0008,0018) | UI | 0020 | 1.2.840.123456.20030822.223344.1
| Hanging Protocol Name | (0072,0002) | SH | 000c | Chest X-ray
| Hanging Protocol Description | (0072,0004) | LO | 0026 | Current and Prior Chest PA and Lateral
| Hanging Protocol Level | (0072,0006) | CS | 0004 | SITE
| Hanging Protocol Creator | (0072,0008) | LO | 0012 | Senior Radiologist
| Hanging Protocol Creation DateTime | (0072,000A) | DT | 000e | 20020823133455
| Hanging Protocol Definition Sequence | (0072,000C) | SQ | ffffffff |
%item |  |  |  |  |
> | Modality | (0008,0060) | CS | 0000 |
> | Anatomic Region Sequence | (0008,2218) | SQ | ffffffff |
%item |  |  |  |  |
>> | Code Value | (0008,0100) | SH | 0008 | 51185008
>> | Coding Scheme Designator | (0008,0102) | SH | 0004 | SCT
>> | Code Meaning | (0008,0104) | LO | 0006 | Chest
%enditem |  |  |  |  |
%endseq |  |  |  |  |
> | Procedure Code Sequence | (0008,1032) | SQ | 0000 |
> | Laterality | (0020,0060) | CS | 0000 |
> | Reason for Requested Procedure Code Sequence | (0040,100A) | SQ | 0000 |
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Hanging Protocol User Identification Code Sequence | (0072,000E) | SQ | 0000 |
| Number of Priors Referenced | (0072,0014) | US | 0002 | 1
| Number of Screens | (0072,0100) | US | 0002 | 0002H
| Nominal Screen Definition Sequence | (0072,0102) | SQ | ffffffff |
%item |  |  |  |  |
> | Number of Vertical Pixels | (0072,0104) | US | 0002 | 2560
> | Number of Horizontal Pixels | (0072,0106) | US | 0002 | 2048
> | Display Environment Spatial Position | (0072,0108) | FD | 0020 | 0.0\1.0\0.5\0.0
> | Screen Minimum Grayscale Bit Depth | (0072,010A) | US | 0002 | 0008H
> | Application Maximum Repaint Time | (0072,010E) | US | 0002 | 0064H
%enditem |  |  |  |  |
%item |  |  |  |  |
> | Number of Vertical Pixels | (0072,0104) | US | 0002 | 2560
> | Number of Horizontal Pixels | (0072,0106) | US | 0002 | 2048
> | Display Environment Spatial Position | (0072,0108) | FD | 0020 | 0.5\1.0\1.0\0.0
> | Screen Minimum Grayscale Bit Depth | (0072,010A) | US | 0002 | 0008H
> | Application Maximum Repaint Time | (0072,010E) | US | 0004 | 0064H
%enditem |  |  |  |  |
%endseq |  |  |  |  |

C-FIND Response #3:

Nesting | Attribute | Tag | VR | VL (hex) | Value
--- | --- | --- | --- | --- | ---
| Affected SOP Class UID | (0000,0002) | UI | 0018 | 1.2.840.10008.5.1.4.38.2
| Command Field | (0000,0100) | US | 0002 | 8020H [C-FIND-RSP]
| Message ID Being Responded To | (0000,0120) | US | 0002 | 0010H
| Data Set Type | (0000,0800) | US | 0002 | 0102H
| Status | (0000,0900) | US | 0002 | FF00H [Pending]
| SOP Class UID | (0008,0016) | UI | 0018 | 1.2.840.10008.5.1.4.38.1
| SOP Instance UID | (0008,0018) | UI | 002a | 1.2.840.113986.2.664566.21121125.85669.967
| Hanging Protocol Name | (0072,0002) | SH | 0010 | Chest X-ray_LGon
| Hanging Protocol Description | (0072,0004) | LO | 003e | Prior and Current Lateral of Chest X-ray for two screen system
| Hanging Protocol Level | (0072,0006) | CS | 000c | SINGLE_USER
| Hanging Protocol Creator | (0072,0008) | LO | 0012 | Dr. Leia Gonzales
| Hanging Protocol Creation DateTime | (0072,000A) | DT | 000e | 20030822101100
| Hanging Protocol Definition Sequence | (0072,000C) | SQ | ffffffff |
%item |  |  |  |  |
> | Modality | (0008,0060) | CS | 0002 | DX
> | Anatomic Region Sequence | (0008,2218) | SQ | ffffffff |
%item |  |  |  |  |
>> | Code Value | (0008,0100) | SH | 0008 | 51185008
>> | Coding Scheme Designator | (0008,0102) | SH | 0004 | SCT
>> | Code Meaning | (0008,0104) | LO | 0006 | Chest
%enditem |  |  |  |  |
%endseq |  |  |  |  |
> | Procedure Code Sequence | (0008,1032) | SQ | 0000 |
> | Laterality | (0020,0060) | CS | 0000 |
> | Reason for Requested Procedure Code Sequence | (0040,100A) | SQ | 0000 |
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Hanging Protocol User Identification Code Sequence | (0072,000E) | SQ | 0000 |
%item |  |  |  |  |
> | Code Value | (0008,0100) | SH | 0004 | Lgon
> | Coding Scheme Designator | (0008,0102) | SH | 0008 | 99Local
> | Coding Scheme Version | (0008,0103) | SH | 0004 | v40a
> | Code Meaning | (0008,0104) | LO | 000c | log-in name
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Number of Priors Referenced | (0072,0014) | US | 0002 | 1
| Number of Screens | (0072,0100) | US | 0002 | 0002H
| Nominal Screen Definition Sequence | (0072,0102) | SQ | ffffffff |
%item |  |  |  |  |
> | Number of Vertical Pixels | (0072,0104) | US | 0002 | 1280
> | Number of Horizontal Pixels | (0072,0106) | US | 0002 | 1024
> | Display Environment Spatial Position | (0072,0108) | FD | 0020 | 0.0\1.0\0.5\0.0
> | Screen Minimum Grayscale Bit Depth | (0072,010A) | US | 0002 | 0008H
> | Application Maximum Repaint Time | (0072,010E) | US | 0004 | 0064H
%enditem |  |  |  |  |
%item |  |  |  |  |
> | Number of Vertical Pixels | (0072,0104) | US | 0002 | 1280
> | Number of Horizontal Pixels | (0072,0106) | US | 0002 | 1024
> | Display Environment Spatial Position | (0072,0108) | FD | 0020 | 0.5\1.0\1.0\0.0
> | Screen Minimum Grayscale Bit Depth | (0072,010A) | US | 0002 | 0008H
> | Application Maximum Repaint Time | (0072,010E) | US | 0004 | 0064H
%enditem |  |  |  |  |
%endseq |  |  |  |  |

C-FIND Response #4:

Nesting | Attribute | Tag | VR | VL (hex) | Value
--- | --- | --- | --- | --- | ---
| Affected SOP Class UID | (0000,0002) | UI | 0018 | 1.2.840.10008.5.1.4.38.2.
| Command Field | (0000,0100) | US | 0002 | 8020H [C-FIND-RSP]
| Message ID Being Responded To | (0000,0120) | US | 0002 | 0010H
| Data Set Type | (0000,0800) | US | 0002 | 0101H
| Status | (0000,0900) | US | 0002 | 0000H [Success]

Prev | Up | Next
V.4.3 Hanging Protocol Display Module | Home | V.6 Display Set Patient Orientation Example

DICOM PS3.17 2019e - Explanatory Information