DICOM PS3.17 2019e - Explanatory Information

S.2.2 DNS Server (Current)
Prev | S.2 Managed Association Requester, Legacy Association Acceptor | Next

### S.2.2 DNS Server

The legacy Association Acceptor hostname and IP address should be manually placed into the DNS database.

Prev | Up | Next
S.2 Managed Association Requester, Legacy Association Acceptor | Home | S.2.3 LDAP Server

DICOM PS3.17 2019e - Explanatory Information