DICOM PS3.11 2019e - Media Storage Application Profiles

E.3.3.3 Icon Images (Current)
Prev | E.3.3 Directory Information in DICOMDIR | Next

#### E.3.3.3 Icon Images

Directory Records of type SERIES or IMAGE may include Icon Images. The icon pixel data shall be as specified in PS3.3 Icon Image Key Definition, and restricted such that Photometric Interpretation (0028,0004) shall be MONOCHROME2 or PALETTE COLOR, Bits Allocated (0028,0100) and Bits Stored (0028,0101) shall be equal to 8, and Rows (0028,0010) and Columns (0028,0011) shall be equal to 64.

Prev | Up | Next
E.3.3.2 Localizer Related Attributes | Home | E.3.4 Other Parameters

DICOM PS3.11 2019e - Media Storage Application Profiles