DICOM PS3.7 2019e - Message Exchange

C.3 Cancel Status Class (Current)
Prev | C Status Type Encoding (Normative) | Next

## C.3 Cancel Status Class

Statuses in this Status Class convey that the operation/notification has been canceled.

### C.3.1 Cancel

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to FE00H.

Prev | Up | Next
C.2 Pending Status Class | Home | C.4 Warning Status Class

DICOM PS3.7 2019e - Message Exchange