DICOM PS3.3 2019e - Information Object Definitions

A.8.4 Multi-frame Grayscale Word Secondary Capture Image IOD (Current)
Prev | A.8 Secondary Capture Image IOD | Next

### A.8.4 Multi-frame Grayscale Word Secondary Capture Image IOD

#### A.8.4.1 Multi-frame Grayscale Word SC Image IOD Description

The Multi-frame Grayscale Word Secondary Capture (SC) Image Information Object Definition (IOD) specifies Grayscale Word images that are converted from a non-DICOM format to a modality independent DICOM format.

This IOD is typically used for screen captured images for modalities that have pixel values greater than 8 bits.

Prev | Up | Next
A.8.3.5 Multi-frame Grayscale Byte SC Image Functional Group Macros | Home | A.8.4.2 Multi-frame Grayscale Word SC Image IOD Entity-Relationship Model

DICOM PS3.3 2019e - Information Object Definitions