DICOM PS3.3 2019e - Information Object Definitions

A.42 Ophthalmic Photography 16 Bit Image IOD (Current)
Prev | A Composite Information Object Definitions (Normative) | Next

## A.42 Ophthalmic Photography 16 Bit Image IOD

This Section defines an Information Object to be used with several types of ophthalmic photographic imaging devices including fundus cameras, slit lamp cameras, scanning laser devices, stereoscopic cameras, video equipment and digital photographic equipment, with16 bit resolution per pixel in each image plane.

### A.42.1 Ophthalmic Photography 16 Bit Image IOD Description

The Ophthalmic Photography 16 Bit Image IOD specifies a single-frame or a multi-frame image acquired on a digital photographic DICOM modality. This IOD can be used to encode single ophthalmic images and other combinations including cine sequences.

Prev | Up | Next
A.41.4.2 Contrast/Bolus Agent Sequence | Home | A.42.2 Ophthalmic Photography 16 Bit Image IOD Entity-Relationship Model

DICOM PS3.3 2019e - Information Object Definitions