DICOM PS3.16 2019e - Content Mapping Resource

C Acquisition Context Module, Protocol and Workflow Context Templates (Normative) (Current)
Prev |  | Next

# C Acquisition Context Module, Protocol and Workflow Context Templates (Normative)

This Annex specifies the content of Templates for Acquisition, Protocol and Workflow Context required by DICOM IODs.

## Templates for Acquisition, Protocol and Workflow Context

### TID 3401 ECG Acquisition Context

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 3401. ECG Acquisition Context

| VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | ---
1 | CODE | DT (10:11345, MDC, "Lead System") | 1 | U |  | BCID 3263 “Electrode Placement Values”
2 | CODE | DT (109054, DCM, "Patient State") | 1 | U |  | BCID 3262 “ECG Patient State Values”
3 | NUMERIC | DT (109055, DCM, "Protocol Stage") | 1 | U |  | UNITS = EV ({stage}, UCUM, "stage")
4 | CODE | DT (109056, DCM, "Stress Protocol") | 1 | U |  | BCID 3261 “Stress Protocols”
5 | NUMERIC | DCID 3690 “ECG Control Variables Numeric” | 1-n | U |  |
6 | TEXT | DCID 3691 “ECG Control Variables Text” | 1-n | U |  |

### TID 3403 Catheterization Acquisition Context

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 3403. Catheterization Acquisition Context

| VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | ---
1 | CODE | EV (129085009, SCT, "Catheterization Procedure Phase") | 1 | U |  | BCID 3250 “Catheterization Procedure Phase”
2 | CODE | EV (109058, DCM, "Contrast Phase") | 1 | U |  | BCID 3600 “Relative Times”
3 | CODE | EV (109059, DCM, "Physiological challenges") | 1 | U |  | BCID 3271 “Hemodynamic Physiological Challenges”
4 | NUMERIC | EV (109060, DCM, "Procedure Step Number") | 1 | U |  | UNITS = EV ({step}, UCUM, "step")
5 | TEXT | EV (121124, DCM, "Procedure Action ID") | 1 | U |  |

### Note

See TID 3100 “Procedure Action” in Annex A for description of Procedure Action ID used in Row 5.

### TID 3450 Cardiac Electrophysiology Acquisition Context

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 3450. Cardiac Electrophysiology Acquisition Context

| VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | ---
1 | CODE | EV (109061, DCM, "EP Procedure Phase") | 1 | U |  | BCID 3254 “Electrophysiology Procedure Phase”
2 | NUM | EV (109060, DCM, "Procedure Step Number") | 1 | U |  | UNITS = EV ({step}, UCUM, "step")
3 | TEXT | EV (109063, DCM, "Pulse train definition") | 1 | U |  |

### TID 3460 Projection Radiography Acquisition Context

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 3460. Projection Radiography Acquisition Context

| VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | ---
1 | CODE | DT (130324, DCM, "Functional condition present during acquisition") | 1-n | U |  | BCID 91 “Functional Condition Present During Acquisition”
2 | CODE | DT (364062005, SCT, "Respiration Observable") | 1 | U |  | BCID 3823 “Respiratory Status”
3 | CODE | DT (276334009, SCT, "Joint position") | 1 | U |  | BCID 92 “Joint Position During Acquisition”
4 | CODE | DT (109132, DCM, "Joint positioning method") | 1 | U |  | BCID 93 “Joint Positioning Method”
5 | CODE | DT (109133, DCM, "Physical force") | 1-n | U |  | BCID 94 “Physical Force Applied During Acquisition”

### TID 3470 NM/PET Acquisition Context

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 3470. NM/PET Acquisition Context

| VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | ---
1 | CODE | DT (109054, DCM, "Patient State") | 1 | M |  | DCID 3101 “Cardiac Procedural State Values”
2 | INCLUDE | BTID 3471 “PET Covariates Acquisition Context” | 1 | U |  |

### TID 3471 PET Covariates Acquisition Context

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 3471. PET Covariates Acquisition Context

| VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | ---
1 | NUMERIC | (14749-6, LN, "Glucose") | 1 | U |  | UNITS = EV (mmol/l, UCUM, "mmol/l")
2 | DATE | (127857, DCM, "Glucose Measurement Date") | 1 | MC | IFF Row 1 is present and does not contain Observation DateTime (0040,A032) |
3 | TIME | (127858, DCM, "Glucose Measurement Time") | 1 | MC | IFF Row 1 is present and does not contain Observation DateTime (0040,A032) |

Content Item Descriptions

Row 2 | Glucose Measurement Date | In an earlier edition of the Standard, an incorrect DCM code was used for this concept, which was already assigned as (109081, DCM, "Prospective gating").
Row 3 | Glucose Measurement Time | In an earlier edition of the Standard, an incorrect DCM code was used for this concept, which was already assigned as (109082, DCM, "Retrospective gating").

### TID 8001 Specimen Preparation

This Template describes a single specimen preparation step.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 8001. Specimen Preparation

| VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | ---
1 | TEXT | EV (121041, DCM, "Specimen Identifier") | 1 | M |  |
2 | TEXT | EV (111724, DCM, "Issuer of Specimen Identifier") | 1 | U |  |
3 | CODE | EV (111701, DCM, "Processing type") | 1 | M |  | DCID 8111 “Specimen Preparation Procedure”
4 | DATETIME | DT (111702, DCM, "DateTime of processing") | 1 | U |  |
5 | TEXT | DT (111703, DCM, "Processing step description") | 1 | U |  |
6 | CODE | DT (111703, DCM, "Processing step description") | 1 | U |  | DCID 8113 “Specimen Preparation Steps”
7 | CODE | DT (17636008, SCT, "Specimen Collection") | 1 | MC | IFF Row 3 Processing Type value is (17636008, SCT, "Specimen Collection") | BCID 8109 “Specimen Collection Procedure”
8 | INCLUDE | DTID 8002 “Specimen Sampling” | 1 | MC | IFF Row 3 Processing Type value is (433465004, SCT, "Specimen Sampling") |
9 | INCLUDE | DTID 8003 “Specimen Staining” | 1 | MC | IFF Row 3 Processing type value is (127790008, SCT, "Staining") |
10 | CODE | DT (430864009, SCT, "Tissue Fixative") | 1 | U |  | BCID 8114 “Specimen Fixatives”
11 | CODE | DT (430863003, SCT, "Embedding medium") | 1 | U |  | BCID 8115 “Specimen Embedding Media”

Content Item Descriptions

Row 1 | For sampling steps (which create a child specimen from a parent), the ID is that of the child specimen. For other preparation steps, the ID of a specimen does not change during the processing.
Row 2 | The issuer shall be formatted in accordance with the HL7v2 Hierarchic Designator Data Type. That format is [ Namespace ID]^[ Universal ID^ Universal ID Type], where Namespace IDidentifies an entity within the local namespace or domain, Universal IDis a universal or unique identifier for an entity, and Universal ID Typespecifies the standard format of the Universal ID (see HL7 v2 Section 2.A.33).

### TID 8002 Specimen Sampling

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 8002. Specimen Sampling

| VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | ---
1 | CODE | DT (111704, DCM, "Sampling Method") | 1 | M |  | BCID 8110 “Specimen Sampling Procedure”
2 | TEXT | DT (111705, DCM, "Parent Specimen Identifier") | 1 | M |  |
3 | TEXT | DT (111706, DCM, "Issuer of Parent Specimen Identifier") | 1 | U |  |
4 | CODE | DT (111707, DCM, "Parent specimen type") | 1 | M |  | BCID 8103 “Anatomic Pathology Specimen Types”
5 | TEXT | DT (111708, DCM, "Position Frame of Reference") | 1 | U |  |
6 | TEXT | DT (111709, DCM, "Location of sampling site") | 1 | U |  |
7 | NUMERIC | DT (111710, DCM, "Location of sampling site X offset") | 1 | U |  |
8 | NUMERIC | DT (111711, DCM, "Location of sampling site Y offset") | 1 | U |  |
9 | NUMERIC | DT (111712, DCM, "Location of sampling site Z offset") | 1 | U |  |
10 | IMAGE | DT (111709, DCM, "Location of sampling site") | 1 | U |  |

Content Item Descriptions

Row 3 | The Issuer of Specimen Identifier shall be formatted in accordance with the HL7 v2 Hierarchic Designator data type (see HL7 v2.6 Section 2.A.33), i.e., [ Namespace ID]^[ Universal ID^Universal ID Type]
Row 5 | Description of coordinate system and origin reference point on parent specimen or parent specimen container used for localizing the sampling site
Rows 7-9 | The X, Y and Z locations are used as needed to describe the sampling site; not all may be needed. E.g., resection from 10 cm along the colon may be described as only a Y dimension location.
Row 10 | Reference to image of parent specimen localizing the sampling site; may include referenced Presentation State object

### TID 8003 Specimen Staining

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 8003. Specimen Staining

| VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | ---
1 | CODE | DT (424361007, SCT, "Using substance") | 1-n | MC | IF Row 2 not present | DCID 8112 “Specimen Stains”
2 | TEXT | DT (424361007, SCT, "Using substance") | 1 | MC | IF Row 1 not present |

### TID 8004 Specimen Localization

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 8004. Specimen Localization

| VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | ---
1 | TEXT | DT (111708, DCM, "Position Frame of Reference") | 1 | U |  |
2 | TEXT | DT (111718, DCM, "Location of Specimen") | 1 | U |  |
3 | NUMERIC | DT (111719, DCM, "Location of Specimen X offset") | 1 | U |  |
4 | NUMERIC | DT (111720, DCM, "Location of Specimen Y offset") | 1 | U |  |
5 | NUMERIC | DT (111721, DCM, "Location of Specimen Z offset") | 1 | U |  |
6 | IMAGE | DT (111718, DCM, "Location of Specimen") | 1 | U |  |
7 | COMPOSITE | DT (111718, DCM, "Location of Specimen") | 1 | U |  | Presentation State SOP Instance reference
8 | TEXT | DT (111723, DCM, "Visual Marking of Specimen") | 1 | U |  |

Content Item Descriptions

Row 1 | Description of coordinate system and origin reference point used for localizing the Specimen. The value "CURRENT IMAGE " identifies the frame of reference as the pixel space of the Image SOP Instance in which this Content Item occurs.
Row 2 | Description of specimen location, either in absolute terms or relative to the Position Frame Reference of Row 1
Rows 3-5 | Location of specimen (nominal center) relative to the Position Frame Reference of Row 1. The Content Items include the units of measurement (e.g., mm). If Row 1 value is "CURRENT IMAGE ", measurement shall be from the top left hand corner of the Pixel Data of the SOP Instance, using units of ({pixel}, UCUM, "Pixels").
Row 6 | Reference to image of container localizing the specimen; may include referenced Presentation State object
Row 7 | Reference to Presentation State object for this SOP Instance, with annotations localizing the specimen
Row 8 | Description of visual distinguishing identifiers, e.g., ink, or a particular shape of the specimen

### TID 8010 Slide Imaging Parameters

This Template describes protocol parameters for a Slide Imaging Procedure Step. As an extensible Template, additional items may be included using other concept names from standard or private coding schemes.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 8010. Slide Imaging Parameters

| VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | ---
1 | CODE | EV (112706, DCM, "Illumination Method") | 1-n | U |  | DCID 8123 “Microscopy Illumination Method”
2 | NUMERIC | EV (112707, DCM, "Number of focal planes") | 1 | UC | XOR Row 3 | UNITS = EV ({planes}, UCUM, "planes")
3 | CODE | EV (112707, DCM, "Number of focal planes") | 1 | UC | XOR Row 2 | DT (112714, DCM, "Multiple planes")
4 | NUMERIC | EV (112708, DCM, "Focal plane Z offset") | 1-n | U |  | UNITS = EV (um, UCUM, "um")
5 | CODE | EV (112709, DCM, "Magnification selection") | 1 | U |  | DCID 8132 “Magnification Selection”
6 | NUMERIC | EV (112710, DCM, "Illumination wavelength") | 1-n | U |  | UNITS = EV (nm, UCUM, "nm")
7 | CODE | EV (112711, DCM, "Illumination spectral band") | 1-n | U |  | DCID 8122 “Microscopy Illuminator and Sensor Color”
8 | CODE | EV (112712, DCM, "Optical filter type") | 1-n | U |  | DCID 8124 “Microscopy Filter”
9 | CODE | EV (112713, DCM, "Tissue selection method") | 1 | U |  | DCID 8133 “Tissue Selection”

### TID 8200 Radiology Reading Task Parameters

This Template describes parameters for a radiology reading task.

### Note

Specialty to Read is nested inside Modality to Read in order to facilitate C-FIND matching against both Modality and Specialty.

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 8200. Radiology Reading Task Parameters

| NL | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | ---
1 |  | CODE | EV (128002, DCM, "Modality to Read") | 1 | U |  | DCID 29 “Acquisition Modality”
2 | > | CODE | EV (128003, DCM, "Reader Specialty") | 1 | U |  | DCID 7449 “Reader Specialty”
3 |  | CODE | EV (128004, DCM, "Modality to Read") | 1-n | U |  | DCID 9233 “Requested Report Types”

### TID 15100 Contrast Agent/Pre-Medication Protocol Context

This Template specifies medications to be administered prior to a diagnostic imaging protocol, imaging contrast agents to be used in the protocol, and/or bolus agents to be used in the protocol. Each medication or agent may be modified by a specified route of administration. The top level Content Items of this Template may appear in any order in the Protocol Context Sequence, hence the order in this Template is not significant. There may be significance in the order in which the Content Items are included in the Protocol Context Sequence, e.g., the requested order in which pre-medications are to be administered.

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 15100. Contrast Agent/Pre-Medication Protocol Context

| NL | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | ---
1 |  | CODE | EV (123011, DCM, "Contrast/Bolus Agent") | 1-n | U |  | BCID 12 “Radiographic Contrast Agent”
2 | > | CODE | EV (410675002, SCT, "Route of Administration") | 1 | U |  | BCID 11 “Route of Administration”
3 |  | CODE | EV (123012, DCM, "Pre-Medication") | 1-n | U |  |
4 | > | CODE | EV (410675002, SCT, "Route of Administration") | 1 | U |  | BCID 11 “Route of Administration”

### TID 15101 NM/PET Protocol Context

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 15101. NM/PET Protocol Context

| NL | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | ---
1 |  | CODE | EV (349358000, SCT, "Radiopharmaceutical agent") | 1 | M |  | BCID 25 “Radiopharmaceuticals” BCID 4021 “PET Radiopharmaceutical”
2 | > | CODE | EV (89457008, SCT, "Radionuclide) | 1 | U |  | BCID 18 “Isotopes in Radiopharmaceuticals” BCID 4020 “PET Radionuclide”
3 | > | UIDREF | EV (113503, DCM, "Radiopharmaceutical Administration Event UID") | 1 | U |  |
4 | > | DATETIME | EV (123003, DCM, "Radiopharmaceutical Start DateTime") | 1 | U |  |
5 | > | DATETIME | EV (123004, DCM, "Radiopharmaceutical Stop DateTime") | 1 | U |  |
6 | > | NUMERIC | EV (123005, DCM, "Radiopharmaceutical Volume") | 1 | U |  | UNITS = DT (cm3, UCUM, "cm3")
7 | > | NUMERIC | EV (123006, DCM, "Radionuclide Total Dose") | 1 | U |  | UNITS = DT (Bq, UCUM, "Bq")
8 | > | NUMERIC | EV (123007, DCM, "Radiopharmaceutical Specific Activity") | 1 | U |  | UNITS = DT (Bq/mol, UCUM, "Bq/mol")
9 | > | CODE | EV (410675002, SCT, "Route of Administration") | 1 | U |  | BCID 11 “Route of Administration”
10 | > | NUMERIC | EV (123009, DCM, "Radionuclide Syringe Counts") | 1 | U |  | UNITS = DT ({counts}/s, UCUM "counts/s")
11 | > | NUMERIC | EV (123010, DCM, "Radionuclide Residual Syringe Counts") | 1 | U |  | UNITS = DT ({counts}/s, UCUM "counts/s")
12 |  | NUMERIC | EV (14749-6, LN, "Glucose") | 1 | U |  | UNITS = EV (mmol/l, UCUM, "mmol/l")
13 | > | DATE | EV (127857, DCM, "Glucose Measurement Date") | 1 | MC | IFF Row 12 is present and does not contain Observation DateTime (0040,A032) |
14 | > | TIME | EV (127858, DCM, "Glucose Measurement Time") | 1 | MC | IFF Row 12 is present and does not contain Observation DateTime (0040,A032) |

Content Item Descriptions

Row 13 | Glucose Measurement Date | In an earlier edition of the Standard, an incorrect DCM code was used for this concept, which was already assigned as (109081, DCM, "Prospective gating").
Row 14 | Glucose Measurement Time | In an earlier edition of the Standard, an incorrect DCM code was used for this concept, which was already assigned as (109082, DCM, "Retrospective gating").

### TID 15200 JJ1017 Protocol Context

This Template defines protocol context concepts to support the requirements of Japanese Guideline JJ1017. This is expected to be used with Scheduled or Performed Protocol Codes from Coding Scheme JJ1017-16M defined in Guideline JJ1017.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 15200. JJ1017 Protocol Context

| NL | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | ---
1 |  | CODE | EV (123016, DCM, "Imaging Conditions") | 1 | M |  | Baseline terms from Coding Scheme JJ1017-16S of JJ1017 version 3.0

### TID 15300 RT Prescription Annotation

The concepts in this TID are topics of advice or information provided by the prescribing physician for planning, preparation and delivery of treatment for a prescription.

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 15300. RT Prescription Annotation

| NL | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | ---
1 | TEXT | EV (130022, DCM, "Radiation Characteristics Note") | 1 | U |  |  |
2 | TEXT | EV (130023, DCM, "Beam Shaping Note") | 1 | U |  |  |
3 | TEXT | EV (130024, DCM, "Treatment Planning Note") | 1 | U |  |  |
4 | TEXT | EV (130025, DCM, "Special Procedure Note") | 1 | U |  |  |
5 | TEXT | EV (130026, DCM, "Patient Positioning Note") | 1 | U |  |  |
6 | TEXT | EV (130028, DCM, "Patient Setup Note") | 1 | U |  |  |
7 | TEXT | EV (130029, DCM, "Previous Treatment Note") | 1 | U |  |  |
8 | TEXT | EV (130030, DCM, "Planning Imaging Note") | 1 | U |  |  |
9 | TEXT | EV (130031, DCM, "Delivery Verification Note") | 1 | U |  |  |
10 | TEXT | EV (130032, DCM, "Simulation Note") | 1 | U |  |  |
11 | CODE | DT (130033, DCM, "Radiation Therapy Particle") | 1-n | U |  |  | BCID 9525 “Radiation Therapy Particle”
12 | CODE | DT (130037, DCM, "Ion Therapy Particle") | 1-n | U |  |  | BCID 9526 “Ion Therapy Particle”
13 | CODE | DT (130038, DCM, "Brachytherapy Isotope") | 1-n | U |  |  | BCID 9528 “Brachytherapy Isotope”
14 | CODE | DT (130040, DCM, "Teletherapy Isotope") | 1-n | U |  |  | BCID 9527 “Teletherapy Isotope”
15 | NUMERIC | DT (130034, DCM, "RT Beam Energy") | 1-n | U |  |  | UNITS=DCID 9521 “Radiotherapy Treatment Energy Unit”
16 | CODE | DT (130035, DCM, "Patient Positioning Procedure Note") | 1-n | U |  |  | BCID 9242 “Radiotherapy Acquisition Workitem Definition”
17 | TEXT | EV (130036, DCM, "QA Process Note") | 1 | U |  |  |
18 | TEXT | EV (130027, DCM, "4D Radiation Treatment Note") | 1 | U |  |  |
19 | TEXT | EV (130039, DCM, "Adaptive Radiation Therapy Note") | 1 | U |  |  |

Content Item Descriptions

Rows 11, 12, 13, 14 | The source of radiation to be used for this RT treatment. More than one source indicates that the RT treatment may use any combination for treatment. There is no defined relationship between the entries in Row 11, 12, 13, 14 and entries in the Rows 15 and 16.
Row 15 | Including several energies indicates that they may be used in any combination.
Row 16 | The codes identify procedures supporting the patient positioning process prior to RT treatment. Including several procedures indicates that they may be used in any combination.

### TID 15301 RT Segment Characteristics

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 15301. RT Segment Characteristics

| NL | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | ---
1 |  | NUMERIC | EV (130082, DCM, "Relative Mass Density") | 1 | U |  | Units = EV (ratio, UCUM, "ratio")
2 |  | NUMERIC | EV (130083, DCM, "Relative Electron Density") | 1 | U |  | Units = EV (ratio, UCUM, "ratio")
3 |  | NUMERIC | EV (130084, DCM, "Effective Z") | 1 | U |  | Units = EV (1, UCUM, "no units")
4 |  | NUMERIC | EV (130085, DCM, "Effective Z per A") | 1 | U |  | Units = EV (/u, UCUM, "/u")
5 |  | NUMERIC | EV (130086, DCM, "Relative Linear Stopping Power") | 1 | U |  | Units = EV (ratio, UCUM, "ratio")
6 | > | NUMERIC | EV (130087, DCM, "Reference Energy") | 1 | M |  | Units = EV (MeV, UCUM, "Megaelectronvolt")
7 |  | NUMERIC | EV (130088, DCM, "Linear Cell Kill Factor") | 1 | U |  | Units = EV (ratio, UCUM, "ratio")
8 |  | NUMERIC | EV (130089, DCM, "Quadratic Cell Kill Factor") | 1 | U |  | Units = EV (ratio, UCUM, "ratio")
9 |  | NUMERIC | EV (130090, DCM, "High Dose Fraction Linear Cell Kill Factor") | 1 | U |  | Units = EV (ratio, UCUM, "ratio")
10 |  | NUMERIC | EV (130091, DCM, "Half-time for Tissue Repair ") | 1 | U |  | Units = EV (s, UCUM, "second")
11 |  | NUMERIC | EV (130092, DCM, "High Dose Fraction Transition Dose") | 1 | U |  | Units = EV (Gy, UCUM, "Gray")
12 |  | NUMERIC | EV (130093, DCM, "Atomic Number") | 1-n | U |  | Units = EV (1, UCUM, "no units")
13 | > | NUMERIC | EV (130094, DCM, "Elemental Composition Atomic Mass Fraction") | 1 | M |  | Units = EV (ratio, UCUM, "ratio")
14 |  | NUMERIC | EV (130095, DCM, "alpha gEUD value") | 1 | U |  | Units = EV (ratio, UCUM, "ratio")

Content Item Descriptions

Rows 12, 13 | The value of (130094, DCM, "Elemental Composition Atomic Mass Fraction") annotates the fractional weight of the elements identified by the (130093, DCM, "Atomic Number") with respect to the total mass of the segment. The allowed value is in the range of [0, 1].

### TID 15302 Patient Support Position Parameters

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 15302. Patient Support Position Parameters

| VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | ---
1 | NUMERIC | EV (126802, DCM, "IEC61217 Table Top Continuous Pitch Angle") | 1 | U |  | Units = EV (deg, UCUM, "deg")
2 | NUMERIC | EV (126803, DCM, "IEC61217 Table Top Continuous Roll Angle") | 1 | U |  | Units = EV (deg, UCUM, "deg")
3 | NUMERIC | EV (126801, DCM, "IEC61217 Patient Support Continuous Yaw Angle") | 1 | U |  | Units = EV (deg, UCUM, "deg")
4 | NUMERIC | EV (126804, DCM, "IEC61217 Table Top Eccentric Axis Distance") | 1 | U |  | Units = EV (mm, UCUM, "mm")
5 | NUMERIC | EV (126805, DCM, "IEC61217 Table Top Continuous Eccentric Angle") | 1 | U |  | Units = EV (deg, UCUM, "deg")
6 | NUMERIC | EV (126806, DCM, "IEC61217 Table Top Lateral Position") | 1 | U |  | Units = EV (mm, UCUM, "mm")
7 | NUMERIC | EV (126807, DCM, "IEC61217 Table Top Longitudinal Position") | 1 | U |  | Units = EV (mm, UCUM, "mm")
8 | NUMERIC | EV (126808, DCM, "IEC61217 Table Top Vertical Position") | 1 | U |  | Units = EV (mm, UCUM, "mm")
9 | NUMERIC | EV (126812, DCM, "Isocentric Patient Support Continuous Pitch Angle") | 1 | U |  | Units = EV (deg, UCUM, "deg")
10 | NUMERIC | EV (126813, DCM, "Isocentric Patient Support Continuous Roll Angle") | 1 | U |  | Units = EV (deg, UCUM, "deg")
11 | NUMERIC | EV (126814, DCM, "Isocentric Patient Support Continuous Yaw Angle") | 1 | U |  | Units = EV (deg, UCUM, "deg")
12 | NUMERIC | EV (126815, DCM, "Isocentric Patient Support Lateral Position") | 1 | U |  | Units = EV (mm, UCUM, "mm")
13 | NUMERIC | EV (126816, DCM, "Isocentric Patient Support Longitudinal Position") | 1 | U |  | Units = EV (mm, UCUM, "mm")
14 | NUMERIC | EV (126817, DCM, "Isocentric Patient Support Vertical Position") | 1 | U |  | Units = EV (mm, UCUM, "mm")

### TID 15303 Radiotherapy Treatment Scheduled Processing Parameters

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 15303. Radiotherapy Treatment Scheduled Processing Parameters

| VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | ---
1 | TEXT | EV (121384, DCM, "RT Plan Label") | 1 | U |  |
2 | NUMERIC | EV (121385, DCM, "Current Fraction Number") | 1 | U |  | UNIT = EV (1, UCUM, "no units")
3 | NUMERIC | EV (121386, DCM, "Number of Fractions Planned") | 1 | U |  | UNIT = EV (1, UCUM, "no units")
4 | NUMERIC | EV (121387, DCM, "Number of Fractions Completed") | 1 | U |  | UNIT = EV (1, UCUM, "no units")
5 | CODE | EV (121388, DCM, "Checked-In Status") | 1 | U |  | DCID 230 “Yes-No”

### TID 15304 Radiotherapy Treatment Progress Parameters

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 15304. Radiotherapy Treatment Progress Parameters

| VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | ---
1 | NUMERIC | EV (121389, DCM, "Referenced Beam Number") | 1 | U |  | UNIT = EV (1, UCUM, "no units")

### TID 15400 Real-World Quantity Definition

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 15400. Real-World Quantity Definition

| NL | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | ---
1 |  | CODE | DT (246205007, SCT, "Quantity") | 1 | M |  | BCID 7180 “Abstract Multi-dimensional Image Model Component Semantics”
2 |  | CODE | BCID 9000 “Physical Quantity Descriptors” | 1-n | U |  |

Content Item Descriptions

Row 1 | This row uses a concept name that specifies the quantified characteristic. It is not required that (246205007, SCT, "Quantity") be used if there is a reason to use a similar concept.
Row 2 | May be concept modifiers, such as (370129005, SCT, "Measurement Method").

### TID 15401 Real-World Quantity Definition for X-Ray Attenuation Properties

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 15401. Real-World Quantity Definition for X-Ray Attenuation Properties

| NL | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | ---
1 |  | INCLUDE | DTID 15400 “Real-World Quantity Definition” | 1 | M |  |
2 |  | NUMERIC | EV (DCM, 130087, "Reference Energy") | 1 | MC | IF TID 15400 Row 1 Quantity value is (130086, DCM, "Relative Linear Stopping Power") | UNITS = EV ("MeV", UCUM, "Megaelectronvolt")

Prev |  | Next
CID 12307 Cardiac Phases and Time Points | Home | D DICOM Controlled Terminology Definitions (Normative)

DICOM PS3.16 2019e - Content Mapping Resource