DICOM PS3.17 2019e - Explanatory Information

XXX.3 Use Cases (Current)
Prev | XXX Volumetric Presentation States (Informative) | Next

## XXX.3 Use Cases

This section includes examples of volumetric views and how they can be described with the Volumetric Presentation States to allow recreation of those views on other systems. The illustrated use cases are examples only and are by no means exhaustive.

Each use case is structured in three sections:

1. User Scenario: Describes the user needs in a specific clinical context, and/or a particular system configuration and equipment type.

2. Encoding Outline: Describes the Volumetric Presentation States related to this scenario, and highlights key aspects.

3. Encoding Details: Provides detailed recommendations of the key Attributes of the Volumetric Presentation States to address this particular scenario. The tables are similar to the IOD tables of PS3.3. Only Attributes with specific recommendation in this particular scenario have been included.

### XXX.3.1 Simple Planar MPR View

#### XXX.3.1.1 User Scenario

A grayscale planar MPR view created from one input volume without cropping is the most basic application of the Planar MPR VPS.

#### XXX.3.1.2 Encoding Outline

To create this view, the Volumetric Presentation State Relationship Module refers to one input volume, and uses the Volumetric Presentation State Display Module with a minimum set of Attributes, generating this simple pipeline:

Figure XXX.3.1-1. Simple Planar MPR Pipeline

The parameters for computing the Multi-Planar Reconstruction are defined in the Multi-Planar Reconstruction Geometry Module.

#### XXX.3.1.3 Encoding Details

##### XXX.3.1.3.1 Volumetric Presentation State Relationship Module Recommendations

Table XXX.3.1-1. Volumetric Presentation State Relationship Module Recommendations

Attribute Name | Tag | Comment
--- | --- | ---
Volumetric Presentation State Input Sequence | (0070,1201) | Set one item in this sequence.
>Presentation Input Type | (0070,1202) | Set to "VOLUME".
>Referenced Image Sequence | (0008,1140) | Set reference(s) to the image(s) that make up the input volume.
>Window Center | (0028,1050) | Set either Window Center and Window Width or VOI LUT Sequence (0028,3010).
>Window Width | (0028,1051) |
>Crop | (0070,1204) | Set to "NO".

##### XXX.3.1.3.2 Volumetric Presentation State Display Module Recommendations

Table XXX.3.1-2. Volumetric Presentation State Display Module Recommendations

Attribute Name | Tag | Comment
--- | --- | ---
Pixel Presentation | (0008,9205) | Set to "MONOCHROME"
Presentation LUT Shape | (2050,0020) | Set to "IDENTITY" or "INVERSE"

Prev | Up | Next
XXX.2.3 Both Volumetric Presentation States and Linked Static Images | Home | XXX.3.2 Spatially Related Views (e.g., Orthogonal)

DICOM PS3.17 2019e - Explanatory Information