DICOM PS3.11 2019e - Media Storage Application Profiles

H.3.4 Other Parameters (Current)
Prev | H.3 STD-GEN-DVD and STD-GEN-SEC-DVD Profile Classes | Next

### H.3.4 Other Parameters

#### H.3.4.2 Multi-frame JPEG Format

The JPEG encoding of pixel data shall use Interchange Format (with table specification) for all frames.

Prev | Up | Next
H.3.3 Directory Information in DICOMDIR | Home | H.3.5 Security Parameters

DICOM PS3.11 2019e - Media Storage Application Profiles