DICOM PS3.3 2019e - Information Object Definitions

F.5.36 Palette Directory Record Definition (Current)
Prev | F.5 Definition of Specific Directory Records | Next

### F.5.36 Palette Directory Record Definition

The Directory Record is based on the specification of Section F.3. It is identified by a Directory Record Type of Value "PALETTE". Table F.5-36 lists the set of keys with their associated Types for such a Directory Record Type. The description of these keys may be found in the Modules related to the Color Palette IOD. This Directory Record shall be used to reference a Color Palette SOP Instance. This type of Directory Record may reference a Lower-Level Directory Entity that includes one or more Directory Records as defined in Table F.4-1.

Table F.5-36. Palette Keys

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Specific Character Set | (0008,0005) | 1C | Required if an extended or replacement character set is used in one of the keys
Content Label | (0070,0080) | 1 | A label that is used to identify the palette.
Content Description | (0070,0081) | 2 | A description of the content of the palette.
Any other Attribute of the Color Palette IOD | 3 |

### Note

Because Referenced SOP Instance UID in File (0004,1511) may be used as a "pseudo" Directory Record Key (see Table F.3-3), it is not duplicated in this list of keys.

Prev | Up | Next
F.5.35 Stereometric Relationship Directory Record Definition | Home | F.5.37 Implant Directory Record Definition

DICOM PS3.3 2019e - Information Object Definitions