DICOM PS3.14 2020a - Grayscale Standard Display Function

7.3 Reflective Hardcopy Printers (Current)
Prev | 7 The Grayscale Standard Display Function | Next

## 7.3 Reflective Hardcopy Printers

For reflective hardcopy printing, the relationship between luminance, L, and the printed optical density, D, is:

Equation 7-6.

where:

- L0 is the maximum luminance obtainable from diffuse reflection of the illumination that is present.

If film is to be printed with a density ranging from Dmin to Dmax, the final luminance will range between
and
and the j values will correspondingly range from jmin = j(Lmin) to jmax = j(Lmax).

If this span of j values is represented by an N-bit P-Value, ranging from 0 for jmin to 2N-1 for jmax, the j values will correspond to P-Values as follows:

Equation 7-7.

and the corresponding L values will be L(j(p)).

Finally, converting the L(j(p)) values to densities results in

Equation 7-8.

### Note

Typical values for the parameters used in reflective hardcopy printing are L0 = 150 cd/m2.

Prev | Up | Next
7.2 Transmissive Hardcopy Printers | Home | 8 References

DICOM PS3.14 2020a - Grayscale Standard Display Function