DICOM PS3.18 2020a - Web Services

11.8.3.2 Response Header Fields (Current)
Prev | 11.8.3 Response | Next

#### 11.8.3.2 Response Header Fields

The origin server shall support header fields as required in Table 11.8.3-2.

Table 11.8.3-2. Response Header Fields

Name | center | Origin Server Usage | Description
--- | --- | --- | ---
Content-Type | media-type | C | The media type of the Status Report document. Shall be present if the response contains a payload.
Content-Length | uint | C | Shall be present if a content encoding has not been applied to the payload.
Content-Encoding | encoding | C | Shall be present if a content encoding has been applied to the payload.

If the Workitem Instance is already in a canceled state, the response message shall include the following HTTP Warning header field:

    Warning: 299 <service>: The UPS is already in the requested state of CANCELED.

See also Section 8.4.

Prev | Up | Next
11.8.3 Response | Home | 11.8.3.3 Response Payload

DICOM PS3.18 2020a - Web Services