DICOM PS3.4 2020a - Service Class Specifications

FF.2.3.2.2 Compositor Components (Current)
Prev | FF.2.3.2 Description of Display Components | Next

##### FF.2.3.2.2 Compositor Components

There are two compositor component types defined for compositing of two input RGBA (or one RGBA and one RGB) data sources. The defined components are:

- RGB Compositor: This component accepts two RGBA inputs (with one Alpha input optional) and composites the data into a single RGB output. Each item of Presentation State Compositor Component Sequence (0070,1805) specifies one RGB Compositor component:

  Figure FF.2-5. RGB Compositor Component

- RGBA Compositor: This component accepts two RGBA inputs and composites the data into a single RGB output and a single Alpha output.

  Figure FF.2.3.2.2-2. RGBA Compositor Component

Prev | Up | Next
FF.2.3.2 Description of Display Components | Home | FF.2.3.3 Internal Structure of Components

DICOM PS3.4 2020a - Service Class Specifications