DICOM PS3.2 2020a - Conformance

J.4.4 Configuration (Current)
Prev | J.4 Networking | Next

### J.4.4 Configuration

#### J.4.4.1 STOW-RS Interface

The EXAMPLE-STOW-SERVICE is configured to respond to TLS protected traffic. The TLS port will refuse any connection from a system that is not recognized as authenticated by a known authority.

Prev | Up | Next
J.4.3.3 IPv4 and IPv6 Support | Home | J.5 Media Interchange

DICOM PS3.2 2020a - Conformance