DICOM PS3.3 2020a - Information Object Definitions

A.34.3.4.6 Sampling Frequency (Current)
Prev | A.34.3.4 12-Lead ECG IOD Content Constraints | Next

##### A.34.3.4.6 Sampling Frequency

The value of Sampling Frequency (003A,001A) in each Waveform Sequence (5400,0100) Item shall be between 200 and 1000, inclusive.

Prev | Up | Next
A.34.3.4.5 Number of Waveform Samples | Home | A.34.3.4.7 Channel Source

DICOM PS3.3 2020a - Information Object Definitions