DICOM PS3.17 2020a - Explanatory Information

XXX.4.3 Ad Hoc Display Layout (Current)
Prev | XXX.4 Uses of Presentation View Description in the Identification Module | Next

### XXX.4.3 Ad Hoc Display Layout

Layout could be accomplished in a display application by using the Presentation Display Collection UID (0070,1101) to identify the presentations to be displayed together, and the View Code Sequence (0054,0220) to determine which presentation to display in each display slot. This requires some clinical context at the exam level, which can be obtained from the source images (for example, Performed Protocol Code Sequence (0040,0260) ).

Prev | Up | Next
XXX.4.2 Structured Displays | Home | XXX.5 Compositing and the Use of Weighting Transfer Functions

DICOM PS3.17 2020a - Explanatory Information