DICOM PS3.3 2020a - Information Object Definitions

C.34.10.2 Dose Notification Triggers (Current)
Prev | C.34.10 Performed CT Acquisition Module | Next

#### C.34.10.2 Dose Notification Triggers

The Computed Tomography Dose Check Standard (NEMA XR-25 athttp://www.nema.org/stds/xr25.cfm) specifies that a Notification Value may be set for the Computed Tomography Dose Index (CTDIvol) and/or the Dose Length Product (DLP) of each Protocol Element. A Dose Check Protocol Element corresponds to an Acquisition Protocol Element in this IOD.

Prev | Up | Next
C.34.10 Performed CT Acquisition Module | Home | C.34.10.3 CT X-Ray Details Sequence

DICOM PS3.3 2020a - Information Object Definitions