DICOM PS3.7 2020a - Message Exchange

C.5.18 No such Event Type (Current)
Prev | C.5 Failure Status Class | Next

### C.5.18 No such Event Type

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Affected SOP Class UID | (0000,0002) | UI | 1 | This optional field contains the SOP Class UID for which the event type does not exist.
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0113H.
Event Type ID | (0000,1002) | US | 1 | This optional field contains the ID of the Event Type that does not exist.

Prev | Up | Next
C.5.17 No such Attribute | Home | C.5.19 No such SOP Instance

DICOM PS3.7 2020a - Message Exchange