DICOM PS3.17 2020a - Explanatory Information

XXX.3.3.3 Encoding Details (Current)
Prev | XXX.3.3 Replacing Set of Derived Images with Multiple Volumetric Presentation States | Next

#### XXX.3.3.3 Encoding Details

##### XXX.3.3.3.1 Volumetric Presentation State Identification Module Recommendations

Table XXX.3.3-1. Volumetric Presentation State Identification Module Recommendations

Attribute Name | Tag | Comment
--- | --- | ---
Presentation Sequence Collection UID | (0070,1102) | Set to the same UID value in each of the Presentation State instances indicating the views are sequentially ordered.
Presentation Sequence Position Index | (0070,1103) | Set to a number indicating the order of each VPS view in the sequentially-ordered set.

Prev | Up | Next
XXX.3.3.2 Encoding Outline | Home | XXX.3.4 Replacing Set of Derived Images With Single VPS Using Crosscurve Animation

DICOM PS3.17 2020a - Explanatory Information