DICOM PS3.4 2020a - Service Class Specifications

B.2.3 Statuses (Current)
Prev | B.2 Behavior | Next

### B.2.3 Statuses

Table B.2-1 defines the specific status code values that might be returned in a C-STORE response. General status code values and fields related to status code values are defined for C-STORE DIMSE Service in PS3.7.

Table B.2-1. C-STORE Status

Service Status | Further Meaning | Status Codes | Related Fields
--- | --- | --- | ---
Failure | Refused: Out of resources | A7xx | (0000,0902)
Error: Data Set does not match SOP Class | A9xx | (0000,0901) (0000,0902)
Error: Cannot understand | Cxxx | (0000,0901) (0000,0902)
Warning | Coercion of Data Elements | B000 | (0000,0901) (0000,0902)
Data Set does not match SOP Class | B007 | (0000,0901) (0000,0902)
Elements Discarded | B006 | (0000,0901) (0000,0902)
Success | Success | 0000 | None

Some Failure Status Codes are implementation specific.

An SCP implementation shall assign specific failure status codes by replacing each 'x' symbol with a hexadecimal digit in the range from 0 to F. An SCP implementation wishing to differentiate between causes within the same Failure Meaning shall assign those causes specific Status Code Values within valid range specified in Table B.2-1.

An SCU implementation shall recognize any Failure Status Code within the value range specified in Table B.2-1 as an indicator of the Failure Meaning stated in the table. There is no requirement for an SCU implementation to differentiate between specific Status Codes within the valid range.

Prev | Up | Next
B.2.2 Behavior of an SCP | Home | B.3 Association Negotiation

DICOM PS3.4 2020a - Service Class Specifications